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Customer:
     
Address:
     
Device Serial #:
     
Creo Contact:
     
Date:
     


Call #:      

Trendsetter 400/800
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Trendsetter 400/800.  Steps that have the greatest impact on system safety and operation appear first in the checklist.

A) Safety and Exterior 

Ensure that the Trendsetter 400/800 is safe to operate and safe to work on.
	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	1. 
	Load glass condition, labels
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	2. 
	Operator interface condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	3. 
	Panels and skins inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	4. 
	Exterior paint check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	5. 
	Compressed air – filters replaced, bowls checked, no leaks 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	6. 
	Air supply pressure test
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	7. 
	Chiller fluid not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	8. 
	Debris cabinet hose not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


B) System Operation 

	Evaluate the current operating condition of the Trendsetter 400/800.

	System Operation
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	· Run diagnostic plot 1, 0 or 100 (repeat diagnostic plot prior to returning Trendsetter to production).

· Submit jobs from workstation

· Watch and listen. Note irregularities for further investigation later.

	9. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	Operator comments summarized below:

	     

	10. 
	Plate exit door 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


C) Imaging

Ensure that the image quality is correct and that the imaging system is operating correctly.

	
	Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	
	Imaging Head
	
	
	
	
	

	11. 
	Test plot assessed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	12. 
	Stroke reference graph generated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	13. 
	Laser power within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	14. 
	Sum and focus error within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	· Remove the thermal imaging head

	15. 
	Debris nozzle checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	16. 
	Lens checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	· Re-install the thermal imaging head

	17. 
	Stroke reference graph generated and compared
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	18. 
	Contrast checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	19. 
	Laser power still within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	20. 
	Shutter opens/closes
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	21. 
	Configuration saved
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Carriage
	
	
	
	
	

	22. 
	Carriage rails lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	23. 
	Carriage lead screw lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	
	Dehumidifier Unit (DHU)
	
	
	
	
	

	24. 
	Filter checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	25. 
	Filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	26. 
	Pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	· If the pressure indicator is red, the DHU MUST be replaced and the air system examined for contaminants.

	
	Debris Removal Unit
	
	
	
	
	

	27. 
	Sensor sends correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	28. 
	Filter in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	29. 
	Hose in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	30. 
	Nozzle and sensor clean and operational
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	31. d
	Data cable in good condition/tight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Chiller/Heat Exchanger
	
	
	
	
	

	32. 
	No leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	33. 
	Hose connections tight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	34. 
	Condenser and air vents cleaned (Chiller only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	35. 
	Pump strainer/ fluid filter cleaned (Chiller only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	36. 
	Pump motor lubricated (Chiller only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	37. 
	Fluid level correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	38. 
	Fans clean and operational (Heat Exchanger only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	· Submit a second test plot for reference.

	
	Image Quality
	
	
	
	
	

	39. 
	Image quality good
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


D) Trendsetter 400/800 

Ensure that the Trendsetter 400/800 system is operating correctly.
	
	Trendsetter 400/800
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	
	Power Box
	
	
	
	
	

	40. 
	Keyswitch operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	41. 
	Power supplies checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	42. 
	Card cage board seating
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Fan Box
	
	
	
	
	

	43. 
	Intake air filters clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	44. 
	Cooling fans – flow and noise check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	45. 
	MOV removed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Engine
	
	
	
	
	

	46. 
	Front panel strut leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	47. 
	Top panel plate door strut leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	48. 
	Exit door actuator condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	49. 
	Load ramp actuators condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	50. 
	Drum and LEC clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	51. 
	Drum straps tight and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	52. 
	Drum belt tension, alignment, condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	53. 
	Glass encoder disk clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	54. 
	Rollers clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	55. 
	Roller actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	56. 
	Roller pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	57. 
	Roller moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	58. 
	Roller rotates smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	59. 
	LEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	60. 
	LEC movement smooth
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	61. 
	LEC gap
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	62. 
	TEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	63. 
	TEC pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	64. 
	TEC magnets clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	65. 
	TEC lock/unlock
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	66. 
	TEC sensor inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	67. 
	Backbone sensors 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	68. 
	Carriage belt tension, inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	69. 
	Main manifold inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	70. 
	Engine timing correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


E) Workstation

Ensure that the configuration is up to date.
	
	Workstation and Controlled Release
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	71. 
	SCSI cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	72. 
	Service Shell at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	73. 
	All firmware at latest version (Head, MPE/MCE, Genine, PDB)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	74. 
	Print Console
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	75. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	76. 
	Test operation
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


F) Creo Service Comments

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed

     
Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	     

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step      
	Date to Complete PM:
	     

	
	Reason:
	     

	
	Plate Count:
	     

	
	
	


	Name of Creo representative:
	     

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	     

	Signature:
	 FORMCHECKBOX 


	Date:
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Customer Support
Tel: 604-451-2727
Toll-free: 800-472-2727
callcentre@creo.com
www.creo.com
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