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Magnus 400 II Family
Planned Maintenance Checklist

The objective of planned maintenance (PM) is to maximize uptime for the Magnus 400 II Family platesetters. Steps that have the greatest impact on system safety and operation appear first in the checklist.

A) Safety and Exterior 

Verify that the Magnus 400 II Family platesetter is safe to operate and safe to work on.
	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	12 Months
	Comments

	1. 
	Operator interface condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	2. 
	Panels and skins inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	3. 
	Exterior paint check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	4. 
	Compressed air – filters replaced, bowls checked, no leaks 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	5. 
	Air supply pressure test
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	6. 
	Coolant not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	7. 
	Debris cabinet hose not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     


B) System Operation 

Evaluate the current operating condition of the Magnus 400 II Family platesetter.
	
	System Operation
	Pass
	Needs
Attn
	12 Months
	Comments

	· Run diagnostics

· Submit jobs from workstation

· Watch and listen. Note irregularities for further investigation later.

	8. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	Operator comments summarized below:

	     


C) Imaging

Verify that the image quality is correct and that the imaging system is operating correctly.

	
	Imaging
	Pass
	Needs
Attn
	12 Months
	Comments

	
	Quantum Imaging Head
	
	
	
	

	9. 
	Test plot assessed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	10. 
	Stroke reference graph generated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	11. 
	Laser power within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	12. 
	Sum and focus error within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	· Remove the thermal imaging head

	13. 
	Debris nozzle checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	14. 
	Lens checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	· Reinstall the thermal imaging head

	15. 
	Stroke reference graph generated and compared
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	16. 
	Contrast checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	17. 
	Laser power still within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	18. 
	Shutter opens/closes
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	19. 
	Configuration saved
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	LDA Imaging Head
	
	
	
	

	20. 
	Laser properly calibrated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Debris Removal Unit
	
	
	
	

	21. 
	Sensor sends correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	22. 
	Filter in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	23. 
	Hose in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	24. 
	Nozzle and sensor clean and operational
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	25. d
	Data cable in good condition/tight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Chiller/Heat Exchanger
	
	
	
	

	26. 
	No leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	27. 
	Hose connections tight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	28. 
	Condenser and air vents cleaned (Chiller only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	29. 
	Pump strainer/ fluid filter cleaned (Chiller only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	30. 
	Pump motor lubricated (Chiller only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	31. 
	Fluid level correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	32. 
	Fans clean and operational (Heat Exchanger only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	· Submit a second test plot for reference

	
	Image Quality
	
	
	
	

	33. 
	Image quality good
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     


D) Back Up Settings and Firmware

Verify that registry and database folders are backed up, and that the Magnus 400 II and Magnus 400 II Quantum firmware is updated.

	
	Back Up Settings and Firmware Evaluation
	Pass
	Needs
Attn
	12 Months
	Comments

	34. 
	Registry ad database folder backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	35. 
	Firmware updated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     


E) Magnus 400 II Family System
Verify that the Magnus 400 II Family system is operating correctly.
	
	Magnus 400 II Family Platesetter
	Pass
	Needs
Attn
	12 Months
	Comments

	
	General
	
	
	
	

	36. 
	All mandatory FCOs implemented and FCO Updater Utility installed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	37. 
	Board functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	38. 
	Loading and unloading systems working properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	39. 
	Drum head and tail grippers working properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	

	40. 
	Drum balance system working properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Loading System (Manual)
	
	
	
	

	41. 
	Loading tray rollers and loading wheel are clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Loading System (MCU II)
	
	
	
	

	42. 
	All detectors are clean and
punch HP detector working properly
All detector screws are securely tightened
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	43. 
	Check punch HP, and adjust accordingly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	44. 
	XY rails are clean and lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	45. 
	XY bar is clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	46. 
	Suction cups in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	47. 
	Paper disposal rollers are clean 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	48. 
	Tweezers replaced
	
	
	
	

	49. 
	Punch slugs vacuumed and punch bin clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Drum System
	
	
	
	

	50. 
	Load gripper, unload gripper, and balance detectors are clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	51. 
	Drum vacuum holes are clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	52. 
	Swivel rotation unit lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	53. 
	Vacuum pump pressure checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Carriage System
	
	
	
	

	54. 
	Carriage HP, fine, and EP detectors clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	55. 
	LDA lens protector secure and clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	56. 
	Light detector clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	57. 
	Oil bracket replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	58. 
	V-block felt lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Unloading System
	
	
	
	

	59. 
	Unload rollers clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	60. 
	Unloading conveyor belt in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Air System
	
	
	
	

	61. 
	Air pressure unit filter replaced by customer every year
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	62. 
	Fans vacuumed clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Vacuum Pump Components
	
	
	
	

	63. 
	Vacuum pump filter replaced. Blades replaced, if required
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	64. 
	Vacuum hoses in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Cooling System (LDA)
	
	
	
	

	65. 
	Strainer is debris‑free 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	66. 
	Coolant refilled regularly by customer
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	67. 
	Heat exchanger is dust-free
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Cooling System (Quantum)
	
	
	
	

	68. 
	Strainer is debris‑free
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	69. 
	Pump in good condition and does not leak
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	70. 
	Reservoir full, in good condition, and does not leak
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	UDRC
	
	
	
	

	71. 
	Particulate filter (BP) or chemical filter (PB, LC) replaced by customer
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Plate Conveyor
	
	
	
	

	72. 
	Ball bearings oiled
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	
	Punch Conveyor
	
	
	
	

	73. 
	Conveyor belts clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	74. 
	Punch slugs vacuumed and punch bin clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	75. 
	Punch conveyor working properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     


F) Workstation

Verify that the configuration is up to date.
	
	Workstation and Controlled Release
	Pass
	Needs
Attn
	12 Months
	Comments

	76. 
	SCSI cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	77. 
	Magnus 400 Controller at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	78. 
	Xpo at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	79. 
	Service Shell at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	80. 
	All firmware at latest version (Head, MPE/MCE, Genine, PDB)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	81. 
	RSS connectivity
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	82. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     

	83. 
	Test operation
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	     


G) Kodak Service Comments

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed

     
Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	     

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step      
	Date to Complete PM:
	     

	
	Reason:
	     

	
	Plate Count:
	     

	
	
	


	Name of Kodak representative:
	     

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	     

	Signature:
	 FORMCHECKBOX 


	Date:
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