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Overview
Upon installation of the Kodak® Magnus™ VLF output device, the Kodak service engineer performs an installation test procedure (ITP), which is a series of tests devised to demonstrate that the installation has been successfully completed and that the output device is fully operational.

The Kodak service engineer must complete this installation test checklist after performing all the test procedures described in the Magnus VLF Installation Test Procedure.

The ITP usually consumes up to ten plates and takes between 2 and 4 hours to complete. During this time, a customer representative must be present to verify the results.

When the tests have been successfully completed, the Magnus VLF is ready for ongoing production work with the full support of the Kodak customer service department.
Customer Responsibilities

The customer is responsible for the following:

· The site must be prepared as described in the Kodak Site Preparation Guide for the device.

· A supply of 25 good quality plates must be available for use in the installation/integration of the output device and the ITP (the ITP uses approximately ten of these plates).

· The processor must be installed and operating.

Kodak Responsibilities

Kodak is responsible for the following:

· The device/system must be fully installed and integrated.

· After installing the Magnus VLF, the Kodak service engineer trains the operator in the operation and maintenance of the device, using the Magnus VLF User Guide or Magnus VLF Visual Quick Reference Guide.

Any additional system, workflow, color calibration, or Staccato® calibration on press are not part of the ITP, and are not covered in this checklist.

Reference Documents

The document numbers listed below are Kodak internal document numbers. The versions indicated may not be the latest version of that document.

	Document Type
	Magnus VLF
	Magnus VLF ContinousLoad (CL)
	Magnus VLF Multi-Cassette Unit (MCU)

	Specifications
	707-00176A
	707-00178A
	707-00177A

	VRGs
	732-00016C
	732-00027C
	732-00014C

	Site Preparation Guide
	725-00032B
	725-00033B
	725-00034B


System Details

	Device serial number
	     

	Head type
	 FORMCHECKBOX 
 Performance
 FORMCHECKBOX 
 Premium

	Resolution
	 FORMCHECKBOX 
 1200 dpi 
 FORMCHECKBOX 
 2540 dpi
 FORMCHECKBOX 
 2400 dpi

	Speed
	 FORMCHECKBOX 
 S
 FORMCHECKBOX 
 F
 FORMCHECKBOX 
 V

	System options
	 FORMCHECKBOX 
 Multi-Cassette Unit(MCU)
 FORMCHECKBOX 
 ContinuousLoad(CL)

	Plate type(s)
	     

	Minimum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Maximum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Workflow
	 FORMCHECKBOX 
 Brisque®
 FORMCHECKBOX 
 Prinergy®
 FORMCHECKBOX 
 Prinergy Evo
 FORMCHECKBOX 
 Third-party TIFF

	
	Version:      

	Screening
(maximum LPI)
	     

	Staccato
(microns)
	     

	Customer punch configured from registered edges
	 FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No


Plate Loading and Unloading
Semiautomatic Plate Loading
Operators should be able to successfully load plates, submit jobs for imaging, and unload plates from the Magnus VLF semiautomatic device.

Completed   FORMCHECKBOX 

Manual Bypass Plate Loading (CL and MCU Devices)
Operators should be able to successfully load plates on the load table extension, submit jobs for imaging, and unload plates from the device. This must be done for single- and dual-plate loading.

Completed  FORMCHECKBOX 

Automatic Plate Loading (MCU Devices)
Operators should be able to successfully load plates into the MCU and submit jobs for imaging. Verify that all plate loading, imaging, and unloading processes are performed automatically. This must be done for single- and dual‑plate loading.

Completed  FORMCHECKBOX 

Plate Throughput

The plate throughput test is designed to verify and demonstrate that the output device meets the specified targets for plate throughput in plates per hour (PPH). The Kodak service engineer exposes several plates, calculates the throughput, and records the results in Table 1.

Table 1: Throughput Test Targets and Results

	Plate size
	PPH (target)
	PPH (measured)

	
	
	     

	
	
	     

	
	
	     

	
	
	     

	
	
	     


Plate Image Quality

To test plate image quality, the Kodak service engineer sends the  Plate Test Target file to the output device, and then inspects a series of test elements on the exposed plate. The test image is shown in Figure 1, and the service engineer records the results of each test element in Table 2 
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Figure 1: Plate Test Target—Image Quality Test Elements for Plates

Table 2 Plate Image Quality Test Results

	Plate Test Target Element
	Description
	Completed

	1. Uniformity patches
	Used for testing the uniformity of the processing line across the plate
	 FORMCHECKBOX 


	2. CTTP test strip
	Used for testing the tone scales
	 FORMCHECKBOX 


	3. Radial vignette 
50% to 100%
	Used to ensure no shade-stepping is present (a smooth transition from 50% to 100%)
	 FORMCHECKBOX 


	4. Radial vignette 
0% to 50%
	Used to ensure no shade-stepping is present (a smooth transition from 0% to 50%)
	 FORMCHECKBOX 


	5. Checkerboard patterns
	Used to verify the image quality of the checkerboard patterns
	 FORMCHECKBOX 


	6. Tone scales
	Visual test to confirm the Staccato screening quality is acceptable with tone scales
	 FORMCHECKBOX 


	7. Vertical and horizontal vignettes
	Used to ensure no shade-stepping is present (a smooth transition from 0% to 100%)
	 FORMCHECKBOX 


	8. Grayscale images
	Used to give the customer an idea of what they can expect when they run their jobs using Staccato screening
	 FORMCHECKBOX 



Confirmation

The installation test was performed on   /   /     (day/month/year) by a representative of Kodak and witnessed by at least one representative of the customer.

	Kodak representative:
	     

	Signature:
	


	Customer representative:
	     

	Signature:
	


Upon completion of this checklist, the Kodak service engineer will send a copy of the entire document to the regional service manager.
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