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Overview

Upon installation of the ThermoFlex® output device, the Kodak service engineer performs an installation test procedure (ITP), which is a series of tests devised to demonstrate that the installation has been successfully completed and that the output device is fully operational.

The Kodak service engineer must complete this installation test procedure checklist (ITPC) after performing all the test procedures described in the ThermoFlex Installation Test Procedure (internal part number 732-00073A-EN).

The ITP usually consumes up to one full-size plate, (full size based on the ThermoFlex drum dimension) and takes between five and six hours to complete. During this time, a customer representative must be present to verify the results.

When the tests have been successfully completed, the ThermoFlex is ready for ongoing production work with the full support of the Kodak Customer Services department.

Customer Responsibilities

The customer is responsible for the following:

· The site must be prepared as described in the Kodak Site Preparation Guide for the device.

· There must be a sufficient supply of good quality plates.
Note: Digital flexographic plates may not be readable by standard film densitometers, which is why a plate measuring device—such as CC Dot or VipFlex (BetaFlex)—is specified. If a plate measuring device is not available, a densitometer may be substituted only with kodak’s permission.

· The processor must be installed and operating.

It is highly recommended that the customer have a light table close to the ThermoFlex device, for inspecting imaged plates and film.

Kodak Responsibilities

Kodak is responsible for the following:

· The device/system must be fully installed and integrated.

· After installing the ThermoFlex, the Kodak service engineer trains the operator in the operation and maintenance of the device, using the ThermoFlex Mid/Narrow User Guides 
(731-00310A-EN / 731-00298A-EN).

Any additional system, workflow, color calibration on press, creation of bump-up curves, or implementation of the special Kodak screening features such as Maxtone, Hyperflex, and Digicap are not part of the ITP, and are not covered in this checklist.

System Details

	Device serial number
	     

	Device type
	     

	Device option
	     

	Resolution
	 FORMCHECKBOX 
 2400 dpi 
 FORMCHECKBOX 
 2540 dpi
 FORMCHECKBOX 
 Other

	Speed
	 FORMCHECKBOX 
 S
 FORMCHECKBOX 
 F
 FORMCHECKBOX 
 V

	Plate type and
drum speed (rpm)
	Plate type                     Drum speed (rpm)      

	
	Plate type                     Drum speed (rpm)      


	
	Plate type                     Drum speed (rpm)      


	
	Plate type                     Drum speed (rpm)      


	
	Plate type                     Drum speed (rpm)      


	Minimum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Maximum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Workflow
	 FORMCHECKBOX 
 Brisque®

	Version:      

	
	 FORMCHECKBOX 
 Prinergy®
	Version:      

	
	 FORMCHECKBOX 
 TIFF FE
	Version:      

	
	 FORMCHECKBOX 
 Third-party TIFF
	Version:      

	Screening
(maximum LPI)
	      Maximum LPI
      Minimum LPI


Imaging Time Throughput

The throughput test is designed to verify and demonstrate that the output device meets the specified imaging time.
Note: Actual throughput of the ThermoFlex system is operator-dependent due to the manual loading architecture of the device. Therefore only laser imaging time is measured to confirm throughput.
The Kodak service engineer images several plates, calculates the throughput, and records the results in Table 1.

Table 1: Throughput Test Targets and Results

	Plate type
	Imaging time (target)
	Imaging time (measured)

	     
	     
	     

	     
	     
	     

	     
	     
	     

	     
	     
	     


Plate Image Quality

To test plate image quality, the Kodak service engineer sends the ThermoFlex Final Test file to the output device, and then inspects a series of test elements on the exposed plate. The test image is shown in Figure 1, and the service engineer records the results of each test element in Table 2. 
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Figure 1: ThermoFlex Final Test File—Image Quality Test Elements for Plates

Table 2 Plate Image Quality Test Results

	Plate Test Target Element
	Description
	Completed

	1. Raster image
	CMYK raster image file 150 lpi at 2540/2400 dpi. Flexo Angles
	 FORMCHECKBOX 


	2. Vignette
	Used to ensure no shade stepping is present (a smooth transition from 0% to 100%)
	 FORMCHECKBOX 


	3. Cross lines and text from positive to reverse
	Crosses and text for focus and density, need to be same thickness
	 FORMCHECKBOX 


	4. Checkerboards
	Squares should border without any bridges and gaps
	 FORMCHECKBOX 


	5. Lines from positive to reverse
	Lines must be identical and straight
	 FORMCHECKBOX 


	6. Slur and stars targets
	Target reference for dot gain/loss, slur and doubling effects
	 FORMCHECKBOX 


	7. Tonal scale
	Calibration target for gray scale 0-100% without bump curves, TIFF file 150 lpi at 2400/2540 dpi
	 FORMCHECKBOX 


	8. Dmin and 50% dot
	Check Dmin is 0.06 ±1 and 50% dot ±4
	 FORMCHECKBOX 



Confirmation

The installation test was performed on   /   /     (day/month/year) by a representative of Kodak and witnessed by at least one representative of the customer.

	Kodak representative:
	     

	Signature:
	


	Customer representative:
	     

	Signature:
	


Upon completion of this checklist, the Kodak service engineer will send a copy of the entire document to the regional service manager.

Customer Comments for Follow-up
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