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Overview

Upon installation of the Trendsetter® 400/800 III output device, the service engineer performs an installation test procedure (ITP), which is a series of tests devised to demonstrate that the installation has been successfully completed and that the output device is fully operational.

The service engineer must complete this installation test checklist after performing all the test procedures described in the Trendsetter 400/800 III Installation Test Procedure.

The ITP usually consumes up to five plates and takes between 2 and 3 hours to complete. During this time, a customer representative must be present to verify the results.

When the tests have been successfully completed, the Trendsetter 400/800 III is ready for ongoing production work with the full support of the Kodak service department.

Customer Responsibilities

The customer is responsible for the following:

· The site must be prepared as described in the Kodak Site Preparation Guide for the device.

· A supply of 25 good quality plates must be available for use in the installation/integration of the output device and the ITP (the ITP uses approximately five of these plates).

· The processor must be installed and operating.

Kodak Responsibilities

Kodak is responsible for the following:

· The device/system must be fully installed and integrated.

· After installing the Trendsetter 400/800 III, the service engineer trains the operator in the operation and maintenance of the device, using the Trendsetter 400/800 III, Trendsetter AL, or Trendsetter ContinuousLoad, Visual Reference Guide.

Any additional system, workflow, color calibration, or Staccato® screening calibration on press are not part of the ITP, and are not covered in this checklist.

System Details

	Device serial number
	     

	Head type
	 FORMCHECKBOX 
 Performance
 FORMCHECKBOX 
 Premium

	Resolution
	 FORMCHECKBOX 
 2400 dpi 

	Speed
	 FORMCHECKBOX 
 S
 FORMCHECKBOX 
 F
 FORMCHECKBOX 
 V
 FORMCHECKBOX 
 X

	System options
	 FORMCHECKBOX 
 AL
 FORMCHECKBOX 
 CL

	Plate type(s)
	     

	Minimum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Maximum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Workflow
	 FORMCHECKBOX 
 Prinergy®
 FORMCHECKBOX 
 Prinergy Evo
 FORMCHECKBOX 
 Third-party TIFF

	
	Version:      

	Screening
(maximum LPI)
	     

	Staccato®
(microns)
	     

	Customer punch configured from registered edges
	 FORMCHECKBOX 
 Yes
 FORMCHECKBOX 
 No


Plate Throughput

The plate throughput test is designed to verify and demonstrate that the output device meets the specified targets for plate throughput in plates per hour (PPH). The service engineer exposes several plates, calculates the throughput, and records the results in Table 1.

Table 1: Throughput test targets and results

	Plate Size
	Trendsetter Speed
	PPH (target)
	PPH (measured)

	
	
	Base
	AL
	CL
	Base
	AL
	CL

	1030 mm (40.5 in.)
	X-speed – TS800 III
	37
	42
	40
	     
	     
	     

	724 mm (28.5 in.)
	V-speed – TS400 III
	43
	50
	50
	     
	     
	     

	1030 mm (40.5 in.)
	V-speed – TS800 III
	30
	34
	34
	     
	     
	     

	1030 mm (40.5 in.)
	F-speed – TS800 III
	22
	24
	24
	     
	     
	     

	1030 mm (40.5 in.)
	S-speed – TS800 III
	15
	16
	16
	     
	     
	     


Plate Image Quality

To test plate image quality, the service engineer sends the Creo Plate Test Target file to the output device, and then inspects a series of test elements on the exposed plate. The test image is shown in Figure 1, and the service engineer records the results of each test element in Table 2.

[image: image1.jpg]IEENEEEEEE
= et d R LI





Figure 1: Creo Plate Test Target—image quality test elements for plates

Table 2: Plate image quality test results

	Plate Test Target Element
	Description
	Completed

	1. Uniformity patches
	Used for testing the uniformity of the processing line across the plate
	 FORMCHECKBOX 


	2. CTTP test strip
	Used for testing the tone scales
	 FORMCHECKBOX 


	3. Radial vignette 
50% to 100%
	Used to ensure no shade-stepping is present (a smooth transition from 50% to 100%)
	 FORMCHECKBOX 


	4. Radial vignette 
0% to 50%
	Used to ensure no shade-stepping is present (a smooth transition from 0% to 50%)
	 FORMCHECKBOX 


	5. Checkerboard patterns
	Used to verify the image quality of the checkerboard patterns
	 FORMCHECKBOX 


	6. Tone scales
	Visual test to confirm the Staccato screening quality is acceptable with tone scales
	 FORMCHECKBOX 


	7. Vertical and horizontal vignettes
	Used to ensure no shade-stepping is present (a smooth transition from 0% to 100%)
	 FORMCHECKBOX 


	8. Grayscale images
	Used to give the customer an idea of what they can expect when they run their jobs using Staccato screening
	 FORMCHECKBOX 



Confirmation

The installation test was performed on   /   /     (day/month/year) by a representative of Kodak and witnessed by at least one representative of the customer.

	Kodak representative:
	     

	Signature:
	


	Customer representative:
	     

	Signature:
	


Upon completion of this checklist, the service engineer will send a copy of the entire document to the regional service manager.
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