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Overview

After system installation and before leaving the customer site, field engineers must ensure that the operators have been thoroughly trained and can successfully demonstrate or describe the procedures and operations listed in the following checklist.

Tools and Documents

The following tools and documents are required for the on-site operator training:

· Kodak® Trendsetter® Visual Reference Guide (supplied with the output device)

· Trendsetter Output Devices Safety Guide

· Filter order list

· Plates

· Files to send for imaging

Operator Training Checklist

Start with the device turned off and the workstation software not running.

Safety

	 FORMCHECKBOX 

	Ensure that the operator is familiar with the Trendsetter Output Devices Safety Guide (761-00029A) and is aware that it contains more detailed safety-related information than this checklist and the other operator documentation (in particular, the online help and the visual reference guide).

	 FORMCHECKBOX 

	Explain the door safety interlock system.

	
	DANGER: Explain that no one must ever tamper with the safety interlock system or remove non-interlocked service tool secured panels. Otherwise, serious personal injury or death could result, along with possible damage to the equipment.

	 FORMCHECKBOX 

	Laser, mechanical, and electrical safety:

	 FORMCHECKBOX 

	Show the location of the power/emergency stop switch and emergency stop (E-stop) button. 

	 FORMCHECKBOX 

	Ensure that customer has a copy of the Trendsetter Output Devices Safety Guide.


Basic Operation of the Output Device

	 FORMCHECKBOX 

	Indicate where the system power switch is located and turn on the Trendsetter.

	 FORMCHECKBOX 

	Explain why the Trendsetter won’t accept jobs for three minutes after the power is turned on. (The laser is initializing.)

	 FORMCHECKBOX 

	Start the Kodak Print Console software.

	 FORMCHECKBOX 

	Demonstrate how to access, open, and search the electronic help documentation.

	 FORMCHECKBOX 

	Demonstrate the proper way to open and/or remove door panels, including how to unlock the front door from Print Console.

	 FORMCHECKBOX 

	Demonstrate how to turn the output device’s compressed air valve on and off. 

	
	WARNING: The compressed air supply to the Trendsetter device should only be turned off as part of the procedure to replace the compressed air supply particulate filters.
At all other times, the compressed air supply must remain turned on, in order to:
· Keep the thermal imaging head dry

· [AL, CL, and NEWS only] Prevent the unexpected movement of the unload table when the compressed air valve is turned back on. This unexpected movement creates a pinching hazard.
· [AL only] Prevent the unexpected movement of the picker assembly when the plate bay door is open and the compressed air valve is turned back on. This unexpected movement can cause serious injury to anyone who is replacing the picker’s Mylar® film strip at the time.
See the warnings in the “Operator Maintenance” section on page 4 for more information.

	 FORMCHECKBOX 

	Show the location of the main breaker switch behind the power box panel. Explain that resetting this switch is the only reason operators should ever need to remove this panel. 

	 FORMCHECKBOX 

	Explain that if the E-stop button is pressed, even while the device is turned off, it needs to be reset (by rotating it 90° clockwise) before the device can return to normal operation. 
If the E-stop button was pressed while the device was on, a Reinitialize command also needs to be sent from the workstation.

	 FORMCHECKBOX 

	Explain that the device will remember the state it was in when shut down (for example, plate on drum).


Output Device Components

	 FORMCHECKBOX 

	Demonstrate how the spring-loaded leading edge clamps (LECs) hold the leading edge of the plate to the drum.

	 FORMCHECKBOX 

	Demonstrate how the magnetic trailing edge clamps (TECs) hold trailing edge of the plate to the drum.

	AL, CL, and NEWS only:

	 FORMCHECKBOX 

	Show the location of the unload table sensor and explain how it detects when a plate is clear of the unload table.

	AL and NEWS only:

	 FORMCHECKBOX 

	Show the plate ledge and explain the function of the air knife and plate separator teeth.

	NEWS Dual-bay option only:

	 FORMCHECKBOX 

	Explain the operation of the dual-bay separator and support arms


Status Lights

	 FORMCHECKBOX 

	Refer to the Visual Reference Guide to show the location of the output device status lights and describe what they mean.


Imaging Plates Using the Workflow Software

Ensure that the operator knows how to perform the following workflow, Print Console, and plate-loading tasks.
Workflow Tasks
	 FORMCHECKBOX 

	Generate a PPD file.

	 FORMCHECKBOX 

	Set up a process template for plate output.

	 FORMCHECKBOX 

	Set up a hot folder and change hot folder locations.

	 FORMCHECKBOX 

	Queue three files locally from the workstation.

	 FORMCHECKBOX 

	Cancel the second file from the workflow software queue

	 FORMCHECKBOX 

	Hold and release jobs in the queue


Print Console and Plate-Loading Tasks

	 FORMCHECKBOX 

	Use the Connect button to put the device queue online and the Disconnect button to put the device queue offline.

	 FORMCHECKBOX 

	Add and edit plate sizes.

	 FORMCHECKBOX 

	Load a plate, correctly using the plate alignment label (or labels).

	 FORMCHECKBOX 

	Use the Stop button to abort the imaging task in progress.

	AL, CL, and NEWS only:

	 FORMCHECKBOX 

	Select the manual bypass function from Print Console.

	 FORMCHECKBOX 

	Load a plate using manual bypass.

	NEWS only:

	 FORMCHECKBOX 

	Load broadsheet plates.


Operator Maintenance

	 FORMCHECKBOX 

	Explain the importance of effective maintenance and replacement procedures.

	 FORMCHECKBOX 

	Demonstrate how to replace the compressed air supply particulate filters.

	
	WARNING: Turn the compressed air shut-off valve to the off position when working on the air supply filters. Failure to do this before inspecting or replacing a compressed air supply filter will result in the following:

· The presence of high-pressure air in the filter elements and bowl, making disassembly difficult and dangerous, resulting in possible serious injury from flying parts

· A very loud noise that could damage your hearing

	 FORMCHECKBOX 

	Demonstrate how to replace the fan box air intake filter.

	 FORMCHECKBOX 

	Show how to clean the edge detect strip and plate roller, and explain what can be used to clean each one.

	AL only:

	 FORMCHECKBOX 

	Show how to replace the Mylar film strip on the picker.

	
	WARNING: The compressed air supply must remain turned on while anyone is working on the picker assembly, to prevent:

· The picker from dropping by gravity

and/or 

· The picker head/vacuum cup assembly from becoming limp and difficult to work with. 

If the compressed air supply is turned off while someone is working on the picker, a hazard exists, because re-energization of the compressed air supply results in sudden, unexpected movement of the picker assembly, which can seriously injure any body part in its path.

Explain to operators that if they suspect that the compressed air supply has been turned off (for example, because the picker drops by gravity and/or the picker head/vacuum cup assembly becomes limp), they must immediately stop working on the picker and close the access panel before investigating why the device or plant air supply has been interrupted. 

If there is a problem with the plant air supply, operators should lock out the device air supply until it has been restored, and keep the access panel closed until the device air supply has been re-energized. 

	If the output device has a universal debris removal cabinet (UDRC):

	 FORMCHECKBOX 

	Demonstrate how to change the filter (or filters) in the UDRC.


Troubleshooting

Simulate a plate fly-off. Ensure that the operator:

	 FORMCHECKBOX 

	Does not turn off the device or exit the software as a means of error recovery.

	 FORMCHECKBOX 

	Correctly responds to workstation error dialog boxes.

	 FORMCHECKBOX 

	Properly and safely removes the plate from the drum, wearing gloves.

	 FORMCHECKBOX 

	Properly puts trailing edge clamps (TEC) to the park position.

	 FORMCHECKBOX 

	Continues to properly respond to and clear error recovery dialog boxes.


Print a copy of this checklist and leave it with the customer for future reference (for example, when training other operators).


	Customer name:
	     

	Device serial number:
	     

	Operator names:
	     

	
	     

	
	     

	
	     

	
	     

	
	     

	Kodak representative:
	     

	Customer representative:
	     

	Date:
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