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Overview

Upon installation of the Kodak® ThermoFlex® Wide I platesetter, the Kodak service representative performs an installation test procedure (ITP). The ITP is a series of tests designed to demonstrate that the installation was successfully completed, and that the output device is fully operational.

The Kodak service representative must complete this installation test checklist after performing all the test procedures described in the ThermoFlex Wide I Installation Test Procedure.

The ITP usually consumes one full-size flexographic plate and takes between two and three hours to complete. During this time, a customer representative must be present to verify the results.

When the tests are successfully completed, the ThermoFlex Wide I is ready for ongoing production work with the full support of the Kodak customer service department.

Customer Responsibilities

The customer is responsible for the following:

· Preparing the site, as described in the Kodak Site Preparation Guide for the device

· Supplying a sufficient amount of flexographic plates, for use in the installation and integration of the output device and the ITP. (The ITP and integration uses approximately one full size flexographic plate.)

Note: Standard film densitometers may not be able to read digital flexographic plates. Kodak recommends a plate measuring device such as X-Rite® X-RiteDot™ (CC Dot), FAG Vipflex (BetaFlex), QEA® or any other digital flexographic plate reader. If a plate-measuring device is not available, a densitometer may be substituted only with Kodak’s permission.

· Fully installing the processor and ensuring that it is operating

· Supplying a light table close to the ThermoFlex device for inspecting imaged plates and film.

Kodak Responsibilities

Kodak is responsible for the following:

· Fully installing and integrating the device/system

· After installing the ThermoFlex Wide I, training the operator in the operation and maintenance of the device, using the ThermoFlex Wide I Sheet Mode Operator Guide (653-00745A). The Kodak service representative performs this training.

Any additional system, workflow, color calibration, or calibration of the Kodak Staccato® screening on press, creation of bump-up curves, or implementation of the special Kodak screening features such as Maxtone™, Hyperflex™, and Digicap™ are not part of the ITP, and are not covered in this checklist.

System Details

	Device serial number
	     

	Sleeve Option
	     

	Resolution
	 FORMCHECKBOX 
 2400 dpi 

	Speed
	 FORMCHECKBOX 
 F
 FORMCHECKBOX 
 V

	Plate type     
Plate type     
Plate type     
Plate type     
	Drum speed     
Drum speed     
Drum speed     
Drum speed     

	Minimum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Maximum plate size

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     

	Workflow system
	 FORMCHECKBOX 
 Kodak Brisque®                  Version:      
 FORMCHECKBOX 
 Kodak Prinergy®               Version:      
 FORMCHECKBOX 
 Kodak Prinergy Evo™ Version:      
 FORMCHECKBOX 
 Third-party TIFF          Version:      
 FORMCHECKBOX 
 TIFF Front End            Version:      

	Third-party TIFF Type
	     

	Screening
(maximum LPI)
	     


Plate Loading and Unloading

Operators should be able to use the ThermoFlex Wide I device to successfully load plates, submit jobs for imaging, and unload plates.

	Completed
	     


Plate Throughput

The plate throughput test is designed to verify and demonstrate that the output device meets the specified targets for plate throughput in plates per hour (PPH). The Kodak service representative exposes one plate for each media type and thickness, calculates the throughput, and records the results in Table 1.

Note:   Actual throughput of the ThermoFlex Wide I system is operator-dependent due to the manual loading architecture of the machine. Only the laser imaging time is measured to confirm throughput. In addition, all media must be Kodak-approved since imaging speed is dependent upon media sensitivity.

Table 1: Throughput test targets and results

	Plate Size
	Flexographic Plate Type
	Imaging Time

	     
	     
	     

	     
	     
	     

	     
	     
	     

	     
	     
	     


Plate Image Quality

To test plate image quality, the Kodak service representative sends the plate test target file to the output device, and then inspects a series of test elements on the exposed plate. Figure 1 shows the test image. The service representative records the results of each test element in Table 2.
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Figure 1: Plate test target—image quality test elements for plates

Table 2: Plate image quality test results

	Plate Test Target Element
	Description
	Completed

	1. Tonal Scales
	Calibration target for Grey Scale 0-100% without bump curves, TIFF lpi 100, 120, 133, 150 and 175 at 2400 dpi
	 FORMCHECKBOX 


	2. Vignettes
	Used to ensure that no shade stepping is present (a smooth transition from 50% to 100%)
	 FORMCHECKBOX 


	3. Cross lines, diagonal lines from positive to reverse
	Horizontal, Vertical and Diagonal Lines from 0.2 pt to 3.0 pt must be identical and straight. 
	 FORMCHECKBOX 


	4. Checkerboard and Horizontal/Vertical line patterns
	2-pixel, 4-pixel, 8-pixel Checkerboards, Vertical Lines and Horizontal Lines. Used to confirm 50% tint and confirm focus.
	 FORMCHECKBOX 


	5. Fine Text from positive to reverse
	Text from 4 pt to 10 pt. Used to confirm text reproduction.
	 FORMCHECKBOX 


	6. Solid and 50% 8 x 8 Checkerboard lines.
	Used to confirm 50% tint and check mask clearing. Dmin <= 0.1, 50% = 50 +/-4
	 FORMCHECKBOX 



Confirmation

The installation test was performed on   /   /     (day/month/year) by a representative of Kodak and witnessed by at least one representative of the customer.

	Kodak representative:
	     

	Signature:
	


	Customer representative:
	     

	Signature:
	


After completion of this checklist, the Kodak service representative will send a copy of the entire document to the regional service manager.
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