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Overview

Upon installation of the Kodak® Flexcel™ NX Digital Flexographic System, the Kodak service engineer performs an installation test procedure (ITP), which is a series of tests devised to demonstrate that the installation has been successfully completed and that the system is fully operational.

The Kodak service engineer must complete the installation test checklist after performing all the test procedures described in the Flexcel NX Digital Flexographic System Installation Test Procedure.

The ITP usually consumes one Kodak Flexcel NXH digital flexographic plate and two pieces of Flexcel NX thermal imaging layer (TIL) and takes about one hour to complete.

When the tests have been successfully completed, the Flexcel NX Digital Flexographic System is ready for ongoing production work with the full support of the Kodak service department.

Customer Responsibilities

The customer is responsible for the following:

· The site must be prepared as described in the Kodak Site Preparation Guide for the system.

· A supply of one good quality Flexcel plate and two pieces of Flexcel TIL must be available for use in the installation/integration of the NX device and laminator and the ITP. 
Kodak Responsibilities

Kodak is responsible for the following:

· The system must be fully installed and integrated.

· After installing the Flexcel NX Digital Flexographic System, the Kodak service engineer trains the operator in the operation and maintenance of the system, using the Flexcel NX Digital Flexographic System Visual Reference Guide.

Any additional system, workflow, color calibration, or flexographic plate optimization are not part of the ITP, and are not covered in this checklist.
System Details

	Trendsetter NX serial number
	     

	NX Laminator serial number
	     

	All plate sizes

 FORMCHECKBOX 
 mm
 FORMCHECKBOX 
 in.
	     
     
     
     

	Workflow system
	 FORMCHECKBOX 
 Kodak Prinergy®         Version:          
 FORMCHECKBOX 
 Kodak Prinergy Evo™ Version:      
 FORMCHECKBOX 
 Third-party TIFF          

	Screening
(maximum LPI)
	     


TIL Image Quality
To test image quality, the service engineer sends the Flexcel NX Test Target file to the Trendsetter NX imager, and inspects the test elements on the exposed TIL. The test image is show in Figure 1.
[image: image1.png]



Figure 1: Flexcel NX Test Target
· The average density measurements (from 5 readings) on each target strip on the TIL should conform to the following specifications:
· The Dmin density is ≤ 0.10

· The 8 x 8 pixel checkerboard density is 0.42 ±0.02
· The 1 x 15 pixel tint area density is 2.62 ±0.02
Using a 50x or 100x microscope, examine the 2 x 1 pixel dot inside the T80 box to make sure the dots are rectangular and sharp.  See Figure 2 for the pass/fail reference. 
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Pass
Figure 2: Pass/Fail Reference for 2 x 1 Pixel
The service engineer then sends a 60% tint test file to the Trendsetter NX imager, and inspects the uniformity across the exposed TIL.
Lamination Quality

The service engineer laminates the TIL with the 60% tint test image and makes sure that there are no bubbles on the plate after lamination.
Confirmation

The installation test was performed on  COMMENTS   \* MERGEFORMAT   /   /     (day/month/year) by a representative of Kodak and witnessed by at least one representative of the customer.

	Kodak representative:
	     

	Signature:
	


	Customer representative:
	     

	Signature:
	


Upon completion of this checklist, the Kodak service representative will send a copy of the entire document to the regional service manager.
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