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Customer:

Address:

Device Serial #:  
Creo Contact
:  
Date:

Dolev 4Press
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Dolev 4Press.  Steps that have the greatest impact on system safety and operation appear first in the checklist.

Planned maintenance should be performed every 6 months.

A) Safety and Exterior 

Ensure that the Dolev 4Press is safe to operate and safe to work on.
Allow 20 minutes.

	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	1. 
	Site conditions within specifications
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	2. 
	Doors and sides safely interlocked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	3. 
	Panels, doors and covers in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	4. 
	Operating panel and keys in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


B) System Operation 

Evaluate the current operating condition of the Dolev 4Press.
Allow 30-60 minutes.

	
	System Operation
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	5. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	Operator comments summarized below:

	

	6. 
	Operator trained
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	7. 
	Firmware version updated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	8. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	· Film loaded into the drum

	9. 
	Rocker assembly closes smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	10. 
	Loading progresses smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	11. 
	Film is smoothly spread in drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	12. 
	Cutter moves smoothly and cuts evenly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	13. 
	Film unloads smoothly from drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	14. 
	Carriage moves quietly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	15. 
	Dynamic optic chain uncoils and coils smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


C) Imaging 

Ensure that the image quality is correct and that the imaging system is operating correctly.
Allow 1 hour.

	
	Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	Static optic
	
	
	
	
	
	
	

	16. 
	Laser power within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	· Submit a second test plot for reference.

	17. 
	Image quality acceptable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	



D) Dolev 4Press Systems and Components 

Ensure that the Dolev 4Press systems and components are clean, in good condition, and operating correctly.
Allow 3-4 hours.

	
	Systems and Components
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	18. 
	All mandatory FCOs implemented
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	19. 
	All E- and P-box board revision levels updated and boards cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	20. 
	Data box (if exists) clean and VLSI board comp level updated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	21. 
	Machine parameters set according to customer requirements, and saved
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	22. 
	All detectors functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Loading system
	
	
	
	
	
	
	

	23. 
	Loading cassettes clean, film tension per spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	24. 
	Film-in detectors functioning
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	25. 
	Load/unload rollers clean, pressure per spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	26. 
	Cutter clean, lubricated, and chain tension acceptable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	27. 
	Film transport guides clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	28. 
	Unloading cassette clean, no light leakage
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Drum assembly
	
	
	
	
	
	
	

	29. 
	Drum cavity and guide beam clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	30. 
	Drum air release grooves clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	31. 
	Film well attached to drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	32. 
	Feed detectors and counters functioning to spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Carriage/dynamic optic assembly
	
	
	
	
	
	
	

	33. 
	Leadscrew clean, lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	34. 
	Leadscrew coupling pressure within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	35. 
	Dynamic optics clean, including spinner; bow and linearity properly adjusted
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	36. 
	Penta prism/cube clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	37. 
	Fiber connectors clean and connectors lubricated with optic gel
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Punch assembly
	
	
	
	
	
	
	

	38. 
	Punch slugs removed and container cleaned.
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	39. 
	Punch (if exists) clean and lubricated, functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Power supply
	
	
	
	
	
	
	

	40. 
	Power unit voltage levels according to spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


E) Creo Service Comments

Make sure to record PM call information.

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed


Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step 
	Date to complete PM:
	

	
	Reason:
	

	
	Plate count:
	

	
	
	


	Name of Creo representative:
	

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	

	Signature:
	 FORMCHECKBOX 


	Date:
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