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Customer:

Address:

Device Serial #:  
Creo Contact
:  
Date:

Dolev 800
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Dolev 800.  Steps that have the greatest impact on system safety and operation appear first in the checklist.

Planned maintenance should be performed every 6 months.

A) Safety and Exterior 

Ensure that the Dolev 800 is safe to operate and safe to work on.
Allow 20 minutes.

	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	1. 
	Site conditions within specifications
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	2. 
	Doors and upper cover safely interlocked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	3. 
	Panels, doors and covers in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	4. 
	Operating panel and keys in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


B) System Operation 

Evaluate the current operating condition of the Dolev 800.
Allow 30-60 minutes.

	
	System Operation
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	5. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	Operator comments summarized below:

	

	6. 
	Operator trained
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	7. 
	Firmware version updated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	8. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	· Expose a gray scale for reference.

	9. 
	Loading progresses smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	10. 
	Film is smoothly spread in drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	11. 
	Cutter moves smoothly and cuts evenly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	12. 
	Film unloads smoothly from drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	13. 
	Carriage moves quietly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	14. 
	Dynamic optic chain uncoils and coils smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


C) Imaging 

Ensure that the image quality is correct and that the imaging system is operating correctly.
Allow 1 hour.

	
	Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	Static optic
	
	
	
	
	
	
	

	15. 
	Laser power within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	· Submit a second test plot for reference.

	16. 
	Image quality acceptable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


D) Dolev 800 Systems and Components 

Ensure that the Dolev 800 systems and components are clean, in good condition, and operating correctly.
Allow 4-5 hours.

	
	Systems and Components
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	17. 
	All mandatory FCOs implemented
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	18. 
	All board revision levels updated and boards cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	19. 
	Data box (if exists) clean and comp level updated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	20. 
	All detectors functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Loading system
	
	
	
	
	
	
	

	21. 
	Loading cassettes clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	22. 
	Cassette detectors functioning
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	23. 
	Cassette rubber wheels clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	24. 
	Film-in detectors functioning
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	25. 
	Feeding roller Dellerin wheels clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	26. 
	Cutter clean, lubricated, and chain tension acceptable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	27. 
	Feeder wheels clean and pressure acceptable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	28. 
	Film transport guides clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	29. 
	Unloading cassette clean, no light leakage
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Drum assembly
	
	
	
	
	
	
	

	30. 
	Spreader wheels clean, positioned correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	31. 
	Film well attached to drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	32. 
	Drum cavity and central beam clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	33. 
	Drum vacuum holes clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	34. 
	Vacuum pump and valves functioning properly, pressure level correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	35. 
	Feed detectors and counters functioning to spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	36. 
	Spreader motor chain’s rubber wheels and sprockets in good condition, with proper tension
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Carriage/dynamic optic assembly
	
	
	
	
	
	
	

	37. 
	Leadscrew lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	38. 
	Leadscrew coupling pressure within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	39. 
	Dynamic optics clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	40. 
	Spinner encoder (if not under warranty) clean, bow and linearity properly adjusted
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	41. 
	Shutter clean and shutter solonoid functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	42. 
	Penta prism/cube clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	43. 
	Fiber connectors clean and connectors lubricated with optic gel
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Punch assembly
	
	
	
	
	
	
	

	44. 
	Punch (if exists) clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	45. 
	Air supply functioning properly and input pressure to spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	46. 
	Punch functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Power supply
	
	
	
	
	
	
	

	47. 
	Power unit voltage levels to spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


E) Creo Service Comments

Make sure to record PM call information.

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed


Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step 
	Date to complete PM:
	

	
	Reason:
	

	
	Plate count:
	

	
	
	


	Name of Creo representative:
	

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	

	Signature:
	 FORMCHECKBOX 


	Date:
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