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VMR Order Form for Trendsetter 400/800 (MPE) and Trendsetter VLF

This procedure must be completed for ordering 632-00354A—Variable Mainscan Resolution for Trendsetter 3230/3244/400/800/VLF option. 

Follow all the steps starting from STEP 1 to place an order.

	STEP 1
	VERIFY SITE REQUIREMENTS


The following tables provide details of all the possible site requirements for placing an order for VMR.
· Check those boxes that meet the configuration for the particular site situation.
· At least one box should be checked in each table in order to install the VMR option. Otherwise, you must arrange for the appropriate upgrades before proceeding.
Workflow Software Requirements

	Workflow Software
	Verify

	Kodak Brisque 5.1.32 or higher 
	  YES

	Kodak Prinergy 3.0 or higher
	  YES

	Kodak Prinergy Evo 3.0 or higher
	  YES

	3rd Party workflow capable of generating 1-bit TIFF files with asymmetric resolutions 
	  YES


Controlled Release Requirements: 

· In Service Shell client, click Version Checker.
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· Note the Controlled Release version under Release Information.
· If the device Controlled Release is unknown or not qualified, contact CD.Requests@creo.com for the latest Controlled Release CD.
· The part number of the Controlled Release CD for the respective devices can be found at: http://techplanet.creo.com/output/computer_to_plate/all_ctp/nav/control-set.htm) 
	Device
	Controlled Release version
	Verify

	Trendsetter 400/800 Base
	MPE Controlled Release 1.3 or higher
	  YES

	Trendsetter 400/800 AL
	MPE Controlled Release 2.2 or higher
	  YES

	Trendsetter 400/800 Spectrum
	MPE Controlled Release 3.2 or higher
	  YES

	Trendsetter VLF and VLF AL
	MPE Controlled Release 4.1 or higher
	  YES


	STEP 2
	GET SYSTEM ID


· In Print Console, select Configuration>Preferences>Licenses.
· Note the TIFF downloader System ID and enter it in Step 3 below.
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	STEP 3
	FILL OUT THIS FORM


Customer Information:

	Date
	

	Company name
	

	Customer contact name
	

	Your e-mail address
	

	Device serial number
	

	TIFF downloader system ID 
	

	Sales order number
	


	STEP 4
	MAIL OR FAX THIS FORM TO ORDER MANAGEMENT
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