Magnetic Sensor cheater position

MAGNETIC SENSOR Cheater 





The cheater should be place on the corner of the  right bottom of the loading cassette entrance.


As soon as the cheater is attach to the magnetic sensor of the machine,  the interlock in of the cassette  should change status  from On  to  OFF.





Magnet sensor inside the machine








