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Customer:

Address:

Device Serial #:  
Creo Contact
:  
Date:

Lotem 800 Q / II Family
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Lotem 800 Q / II Family. Steps that have the greatest impact on system safety and operation appear first in the checklist.

A) Safety and Exterior 

Ensure that the Lotem 800 Q / II Family is safe to operate and safe to work on.
Allow 10-20 minutes.

	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	1. 
	Site conditions are according to specifications
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	2. 
	Doors, panels and interlocks operate correctly.
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	3. 
	Vacuum hoses not leaking.
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	4. 
	Debris cabinet hose not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


B) System Operation 

Evaluate the current operating condition of the Lotem 800 Q / II Family.
Allow 20-30 minutes.

	
	System Operation
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	5. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	Operator comments summarized below:

	

	6. 
	Operator trained
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	7. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	· Expose a large gray scale in three of the client’s favorite formats.

	8. 
	Loads properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	9. 
	Paper is disposed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	10. 
	Plate holds firmly to drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	11. 
	Head/tail grippers operate correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	12. 
	Carriage moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	13. 
	Plate edge detected
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	14. 
	Expose successful
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	15. 
	Plate unloads from drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	16. P
	Unload system operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


C) Imaging 

Note: To properly assess image quality, the processor should have been serviced and filled with fresh chemistry within the last 24 to 48 hours.

	
	Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	General
	
	
	
	
	
	
	

	17. 
	Laser calibrated correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


D) Assemblies and components 

Ensure that the Lotem 800 Q / II Family system is operating correctly.
Allow 4 hours.

	
	Lotem 800 Q / II Family
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	General
	
	
	
	
	
	
	

	18. 
	All mandatory FCOs implemented
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	19. 
	Board revision levels recorded
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	20. 
	Diagnostics have been run
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	21. 
	Detectors cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	22. 
	Air flow regulators adjusted
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	23. 
	Actuator pistons adjusted
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	24. 
	E-box fans cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	25. 
	Overall system checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Loading/Unloading System
	
	
	
	
	
	
	

	26. 
	Loading/unloading rollers cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	27. 
	XY rails cleaned and lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	28. 
	X and Y belt tensions checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	29. 
	XY bar parallelism checked, and bar cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	30. 
	Suction cups checked for wear
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	31. 
	Head/tail grippers checked and screws tightened
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	32. 
	External conveyor ball bearings oiled
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	33. 
	Paper disposal rollers cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	34. 
	Loading pump air filter checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	35. 
	Internal fans checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Drum System
	
	
	
	
	
	
	

	36. 
	Drum vacuum pump air filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	37. 
	Drum vacuum holes cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	38. 
	Vacuum hoses visually checked for wear or damage
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	39. 
	Edge detection strip cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	40. 
	Intake air filter cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	41. 
	Spring spoilers replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	42. 
	Swivel lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Carriage System
	
	
	
	
	
	
	

	43. 
	Leadscrew cleaned and lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	44. 
	Oil pads for V block cleaned and lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	45. 
	V block and carriage cleaned 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Punch System
	
	
	
	
	
	
	

	46. 
	Punch slugs removed from machine and from slugs box
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	47. 
	Punch HP checked, and screws tightened
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	
	Lotem 800 Quantum
	
	
	
	
	
	
	

	48. 
	UDRC particulate filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	49. 
	Cooling system checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


E) Workstation 

Ensure that the configuration is up to date.
Allow 2 hours.

	
	Workstation and Controlled Release
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	50. 
	SCSI cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	51. 
	TSP cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	52. 
	All Head firmware at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	53. 
	All TMCE firmware at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	54. 
	Xilinx software at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	55. 
	Post software at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	

	56. 
	Boot software at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	


F) Creo Service Comments

Record PM call information.

Fine machine calibration performed.

Note any:

· FCOs installed

· Firmware and software updates installed

· Parts replaced

· Safety features disabled or bypassed

· Operating environment issues


Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step 
	Date to Complete PM:
	

	
	Reason:
	

	
	Plate Count:
	

	
	
	


	Name of Creo representative:
	

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	

	Signature:
	 FORMCHECKBOX 


	Date:
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