

MCU for Lotem 800 Thermal Head Platesetter Reliability Checklist
	Customer’s Name: __________________________________    
	Customer ID: __________________

	Installation date: ____/____/____  (DD/MM/YYYY)    
	Platesetter type: _____________________________      

	Platesetter S/N: _____________   
	MCU S/N: ____________


· All testing is performed by an MCU trained engineer

· Follow the MCU for Lotem 800 II Platesetter Installation Guide posted on TechPlanet

· Read preliminary safety precautions

· Verify that the latest version of Lotem Controller is installed (current version release 3.80.16)

· MCU regional jig kit (part number 510J6L041)

· Order relevant FCOs

	Checklist for actions to be taken:
	Done:

	1.
	MCU to platesetter positioning & leveling 

	1.1
	On the platesetter, verify that the height from the paper clamp operator to the floor, is at least 1005 mm. See page 7-9 of the MCU for Lotem 800 II Platesetter Installation Guide.
Adjust the height if required.
Make sure that the platesetter is level.
Remarks: 
	 FORMCHECKBOX 



	1.2
	Check the position, distance, and parallelism between the MCU and the platesetter.
See pages 22-26 of the MCU for Lotem 800 II Platesetter Installation Guide.
Adjust if required.
Remarks:
	 FORMCHECKBOX 


	1.3
	Verify that the MCU bridge is levelled.
See  pages 27-29 of the MCU for Lotem 800 II Platesetter Installation Guide.
Adjust if required.
Remarks:
	 FORMCHECKBOX 



	1.4
	Verify that the rear, front, left, and right of the MCU is levelled.
See pages 29-31 of the MCU for Lotem 800 II Platesetter Installation Guide.
Adjust if required.
Remarks:
	 FORMCHECKBOX 


	1.5
	Measure the MCU diagonals and make sure they are equal.
See pages 29-31 of the MCU for Lotem 800 II Platesetter Installation Guide.
Adjust if required.
Remarks:
	 FORMCHECKBOX 


	1.6
	Fine tune the levels.
See pages 31 of the MCU for Lotem 800 II Platesetter Installation Guide.
Remarks:
	 FORMCHECKBOX 


	2.
	Platesetter to MCU centering
See pages 10, and 32-37 of the MCU for Lotem 800 II Platesetter Installation Guide.

	2.1
	Verify that the platesetter’s centering system is aligned to the MCU interface cassette centering guides.
See pages 9-10 of the MCU for Lotem 800 II Platesetter Installation Guide.
 Adjust, if required by using MCU centering jig (part number 507E3E656). 
Remarks:
	 FORMCHECKBOX 


	2.2
	Verify that the MCU cassette centering system is aligned to the platesetter MCU interface cantering guides. See page 34 of the MCU for Lotem 800 II Platesetter Installation Guide.
Adjust if required.
Remarks:
	 FORMCHECKBOX 


	2.3
	Check plate centering in the cassettes. Adjust if required by using centering jigs.
See page 35 of the MCU for Lotem 800 II Platesetter Installation Guide.
 Remarks:
	 FORMCHECKBOX 


	2.4
	In Lotem Controller, send in turn, all the cassette trays to the platesetter.
Verify that the cassette pins, for each cassette, are adequately positioned.
Verify that the front of the cassette is parallel to the paper disposal assembly.
See page 36 of the MCU for Lotem 800 II Platesetter Installation Guide.
Adjust if required.
Remarks:
	 FORMCHECKBOX 

 FORMCHECKBOX 

 FORMCHECKBOX 


	3.
	Assemblies and FCOs
See TechPlanet FCO page

	3.1
	Verify that Safety Fuse FCO (512-00508) is implemented. 

Verify that the Mitsubishi speed controller parameters are as follows: #9 = 2.5, #22 = 100 
See Configuring Mitsubishi speed control parameters
Remarks:
	 FORMCHECKBOX 

 FORMCHECKBOX 


	3.2
	Implement FCO #512-00266A – Improving the MCU reliability 

Implement FCO #512-00289A – Improving the Main Cylinder Finger 

Install the FCO updater 

Install the FCOs that are designated as Priority next visit.
Verify that the latest version of Lotem Controller is installed (current version release 3.80.16)
Remarks:
	 FORMCHECKBOX 

 FORMCHECKBOX 

 FORMCHECKBOX 

 FORMCHECKBOX 

 FORMCHECKBOX 



	3.3
	Check that the two tunnel cassette bearing guide screws (on each side) are tightened. 
See page 17 of the MCU for Lotem 800 II Platesetter Installation Guide.
Remarks:
	 FORMCHECKBOX 


	3.4
	Check that the two Phillips screws on the side locking latches (R/L) of the user door are tightened.
Remarks:
	 FORMCHECKBOX 


	3.5
	Check the HP/EP detectors for the cassette valves.
Adjust if required.
Remarks:
	 FORMCHECKBOX 


	3.6
	If installed, remove the upper bridge bearing guide (R/L) 

Remarks:
	 FORMCHECKBOX 


	3.7
	Check micro switches (L/R) of the user door.
Adjust if required.

See the Lotem 800 MCU elevator does not move and no error messages appear troubleshooting document.
Remarks:
	 FORMCHECKBOX 


	3.8
	Check the upper and lower limit switches.
Adjust if required.

Remarks:
	 FORMCHECKBOX 


	3.9
	Check the HP/EP detectors of the main tray cylinder.
Adjust if required.

See Lotem 800 II Main Replacement Procedure
Remarks:
	 FORMCHECKBOX 


	4.
	General:

	4.1
	Lubricate the MCU elevator rails.
See  Lotem 800 Family Planned Maintenance Checklist
Remarks:
	 FORMCHECKBOX 


	4.2
	In the Registry, verify that the main air valve/max. allowed sol activation time (DWORD) = 4294967295

See Lotem 800 II MCU main air valve detector is missing or in an invalid state
Remarks:
	 FORMCHECKBOX 


	5.
	Testing the MCU

	5.1
	Run the MCU test script
Remarks:
	 FORMCHECKBOX 


	5.2 
	Run full diagnostic for the platesetter and MCU 

Remarks:
	 FORMCHECKBOX 


	5.3
	Check that the panels and covers of the entire MCU and platesetter are well closed 

Remarks:
	 FORMCHECKBOX 
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