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ThermoFlex Mid and Narrow
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the ThermoFlex Mid and Narrow platesetters. Steps that have the greatest impact on system safety and operation appear first in the checklist.

A) Safety and Exterior 

Ensure that the ThermoFlex Mid or Narrow is safe to operate and safe to work on.
	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	1. 
	Site conditions checked and appropriate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	2. 
	Doors, panels and interlocks inspected
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	3. 
	Exterior paint checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	4. 
	Compressed air – filters replaced, no leaks 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	5. 
	Air supply pressure tested
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	6. 
	Exterior hoses in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	7. 
	Debris cabinet hose not leaking and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	8. 
	Debris cabinet hours/plate count recorded
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	9. 
	External venting hose extends out of the room (UDRC BP)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


B) System Operation and Imaging
Evaluate the current operating condition of the ThermoFlex Mid or Narrow, and ensure that the image quality is correct and that the imaging system is operating correctly.
	
	Operation and Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	· For ThermoFlex Controller version 1.31.350.002 and later, run board diagnostics (repeat diagnostic plot prior to returning ThermoFlex Mid or Narrow to production).

· Expose an ITP file.
· Watch and listen. Note irregularities for further investigation later.

	10. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	Operator comments summarized below:

	     

	11. 
	ITP file quality accessed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	12. 
	Anti-collision system functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	13. 
	Laser power within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	14. 
	Carriage functioning properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	15. 
	Lens checked for damage, adjusted, and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	16. 
	Drum vacuum secures plate to drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Debris Removal Unit
	
	
	
	
	

	17. 
	Filter in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	18. 
	Belt tension adequate (Fuchs)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	19. d
	Data/signal cable in good condition/tight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


C) ThermoFlex Mid or Narrow Platesetter
Ensure that the ThermoFlex Mid or Narrow system is operating correctly.
	
	ThermoFlex Mid or Narrow platesetter
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	20. 
	Next visit FCOs implemented and FCO utility installed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	21. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	22. 
	DDB factors recorded
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	E-box
	
	
	
	
	

	23. 
	Power supplies checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Fan Box
	
	
	
	
	

	24. 
	L-box filter clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	25. 
	Cooling fans in service door, L-box, E-box, and D-box – flow and noise check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Detectors
	
	
	
	
	

	26. 
	Balance and Carriage HP/EP detectors clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	27. 
	Light detector window clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Load/unload
	
	
	
	
	

	28. 
	Unload roller clean (Mid II only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	29. 
	Unload roller clean (Mid II only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	30. 
	Rollers cleaned and movement/location checked (Offset only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Drum
	
	
	
	
	

	31. 
	Drum surface clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	32. 
	Drum vacuum holes clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	33. 
	Drum vacuum pump pressure correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	34. 
	Vacuum pump (dry) filter replaced, blades checked.
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	35. 
	Internal vacuum hoses in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	36. 
	Swivel rotation unit lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	37. 
	Drum magnet strength tested (magnetic drum only)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Clutch (Mid II)
	
	
	
	
	

	38. 
	Belts tension checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	39. 
	Clutch friction adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Carriage
	
	
	
	
	

	40. 
	Debris removal nozzle clean and position checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	41. 
	Light detector clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	42. 
	Lens protector clean and securely fastened
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	43. 
	Oil bracket and V-block felt clean and lubricated, pads replaced if required
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	44. 
	Leadscrew lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     


D) Workstation

Ensure that the configuration is up to date.
	
	Workstation and Controlled Release
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	45. 
	Cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	46. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	47. 
	Latest software versions implemented
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


E) Kodak Service Comments

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed

     
Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	     

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step      
	Date to Complete PM:
	     

	
	Reason:
	     

	
	Plate Count:
	     

	
	
	


	Name of Kodak representative:
	     

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	     

	Signature:
	 FORMCHECKBOX 


	Date:
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