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Customer:

Address:

Device Serial #:  
Creo Contact
:  
Date:

Magnus 400
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Magnus 400.  Steps that have the greatest impact on system safety and operation appear first in the checklist.

Planned maintenance should be performed every 6 months.

A) Imaging 

Ensure that the image quality is correct and that the imaging system is operating correctly.


	
	Imaging
	Pass
	Needs
Attn
	Comments

	1. 
	Image quality acceptable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	2. 
	Laser properly calibrated (LDA)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	3. 
	Laser graph and power checked (Quantum)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	


B) Safety and Exterior 

Ensure that all the Magnus 400 components are safe to operate and to work on.


	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	Comments

	4. 
	Site conditions within specifications
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	5. 
	Doors, panels, and interlocks in good condition and operating correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	6. 
	Debris cabinet hose in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	7. 
	Cooling fluid not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	


C) Backup Settings and Firmware

Ensure back up of the registry and database folder, and the update of the firmware of the Magnus 400 and Magnus 400 Quantum.


	
	Backup Settings and Firmware Evaluation 
	Pass
	Needs
Attn
	Comments

	8. 
	Registry and database folder backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	9. 
	Firmware updated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	


D)  Assemblies and Components 

Ensure that the Magnus 400 systems and components are clean, in good condition, and operating correctly.


	
	Assemblies and components
	Pass
	Needs
Attn
	Comments

	10. 
	All mandatory FCOs implemented and FCO utility installed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	11. 
	Board functioning properly 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	12. 
	Loading and unloading progresses correctly; drum head and tail grippers and drum balance system working properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Loading system (manual)

	13. 
	Loading tray rollers and loading wheel clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Loading system (MCU)

	14. 
	All detectors clean. Punch HP detector performs, and screws tight 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	15. 
	XY rails cleaned and tunnels lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	16. 
	XY bar clean 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	17. 
	Suction cups in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	18. 
	Paper disposal rollers clean, tweezers replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	19. 
	Punch slugs cleaned away
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Drum system

	20. 
	Load gripper, unload gripper and balance enable detectors clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	21. 
	Drum vacuum holes clean 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	22. 
	Swivel rotation unit lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	23. 
	Vacuum pump pressure checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Carriage system

	24. 
	Carriage HP fine and EP detectors clean. 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	25. 
	Lens protector secure and clean (LDA)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	26. 
	Light detector clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	27. 
	Oil bracket replaced,
V-block felt lubricated 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Unloading system

	28. 
	Unload rollers clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	29. 
	Plate out of drum and plate out of machine detectors clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	30. 
	Unloading conveyor belt in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Air system

	31. 
	Air pressure unit filter replaced by customer every six months
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	32. 
	Fans vacuumed clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Vacuum pump components

	33. 
	Vacuum pump filter replaced. Blades replaced, if required
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	34. 
	Vacuum hoses in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Cooling system (LDA)

	35. 
	Temperature checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	36. 
	Cooling liquid refilled regularly by customer
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	Cooling system (Quantum)

	37. 
	Strainer free of debris
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	38. 
	Pump in good condition and does not leak
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	39. 
	Reservoir full, in good condition, and does not leak
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	UDRC

	40. 
	Particulate filter (BP) or Chemical filter (BP,LC) replaced by customer
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	

	External conveyor

	41. 
	Ball bearings oiled
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	


E) Service Comments

Make sure to record PM call information.

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed


Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step 
	Date to Complete PM:
	

	
	Reason:
	

	
	Plate Count:
	

	
	
	


	Name of Creo representative:
	

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	

	Signature:
	 FORMCHECKBOX 


	Date:
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