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 Screening Escalation Form

ThermoFlex Wide
Note:   Before completing this form, make sure that you have completed the Troubleshooting Flexo Press Artifacts procedure on the TechPlanet Troubleshooting page.

Service Rep Name:      
Customer Name/Number:      

Date:      
ThermoFlex Wide Device Details:
	Number of dead diodes:      
	With no media on the drum and the Z-stage in home position, check for dead diodes using TFX commands:

>>ld all 1000 mw

>>ld all read

>>dps raw range

Attach log files showing results.

	Debris removal system maintenance:
Nozzle cleaned:   FORMCHECKBOX 
  Window cleaned:   FORMCHECKBOX 
  Filter hoses okay:   FORMCHECKBOX 
  Filter okay:   FORMCHECKBOX 


	Describe any artifacts on the unprocessed plate:

     
	Use Flexo ITP file: Flexo-ATP 2400.b.p.1A.K.zip at http://techplanet.creo.com/common/test_files/tfx.htm


Prepress Details:
	Plate type:      
	Plate thickness:      

	RIP used:               Round dot:  FORMCHECKBOX 

	Screen ruling (lpi):      

	CMYK:

C   FORMCHECKBOX 
    M   FORMCHECKBOX 
     Y   FORMCHECKBOX 
    K   FORMCHECKBOX 

	Spot color names:

1        2        3         4       

	Color angles (degrees):

C        M        Y         K       
	Spot angles (degrees):

1        2        3         4       

	Curves applied:       

 COMMENTS  \* MERGEFORMAT 

	Artifact on:

Mask:  FORMCHECKBOX 
                     Processed plate:  FORMCHECKBOX 
                      Press sheet:  FORMCHECKBOX 


	U/V exposure times (minutes):

Main:            Black:                  Post:            Detack:      


Send completed form to:

US&C: jim.third@kodak.com


EAMER: frederic.mayot@kodak.com


You may be asked to send files, plates, and press sheets for evaluation.
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