[image: image2.wmf]


Device Serial #:
     
Date:
     


Trendsetter NEWS
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Trendsetter NEWS.  Steps that have the greatest impact on system safety and operation appear first in the checklist.

A) Safety and Exterior 

Ensure that the Trendsetter NEWS is safe to operate and safe to work on.
Allow 20 minutes.

	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	1. 
	Operator door condition, labels
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	2. 
	Operator interface condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	3. 
	Compressed air – filters replaced, bowls checked, no leaks, no oil, no water 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	4. 
	Air supply pressure
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	5. 
	Warning lights inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	6. 
	Load table inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	7. 
	Picker head condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	8. 
	Unload table/rotator inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	9. 
	Unload table pans condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	10. 
	[Optional] Debris cabinet hose not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


B) System Operation 

Evaluate the current operating condition of the Trendsetter NEWS.
Allow 10-40 minutes. 

	
	System Operation
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	· Run diagnostic plot 1 or 0 or 100 (repeat diagnostic plot prior to returning Trendsetter to production).

· Submit jobs from workstation for automatic loading and manual loading (manual bypass)

· Watch and listen. Note irregularities for further investigation later.

	11. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	Operator comments summarized below:

	     

	12. 
	Lower bay door
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	13. 
	Manual bypass door
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	14. 
	Picker movement
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	15. 
	Picker operations
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	16. 
	Picker vacuum cups
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	17. 
	Plate separator arms
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	18. 
	Plate drop onto pins
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	19. 
	Plate loading onto drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	20. 
	Edge detection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	21. 
	Carriage operation
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	22. 
	Plot operation
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	23. 
	Plate unload from drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	24. 
	Unload table movement
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	25. 
	[Optional] Plate rotator movement
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	26. 
	Plate rotator cups
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


C) Imaging

Ensure that the image quality is correct and that the imaging system is operating correctly.
Allow approximately 1 hour.
	
	Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	
	Carriage
	
	
	
	
	

	27. 
	Carriage rails lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	28. 
	Carriage lead screw lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	     

	
	[Optional] Debris Removal Unit
	
	
	
	
	

	29. 
	Sensor sends correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	30. 
	Filter in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	31. 
	Hose in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	32. 
	Nozzle and sensor clean and operational
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	33. d
	Data cable in good condition/tight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	· Submit a second test plot for reference.

	
	Image Quality
	
	
	
	
	

	34. 
	Image quality good
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


D) Trendsetter NEWS 

Ensure that the Trendsetter NEWS system is operating correctly.
Allow 2 hours. 

	
	Trendsetter base
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	
	Power Box
	
	
	
	
	

	35. 
	Keyswitch operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Fan Box
	
	
	
	
	

	36. 
	Intake air filters clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	37. 
	Cooling fans – flow and noise check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Engine
	
	
	
	
	

	38. 
	Front panel strut leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	39. 
	AL plate door strut leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	40. 
	Load ramp actuators condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	41. 
	Drum and LEC clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	42. 
	Drum straps tight and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	43. 
	Drum belt condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	44. 
	Rollers clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	45. 
	Roller actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	46. 
	Roller pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	47. 
	Roller moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	48. 
	Roller rotates smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	49. 
	LEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	50. 
	LEC movement smooth
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	51. 
	LEC gap
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	52. 
	TEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	53. 
	TEC pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	54. 
	TEC magnets clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	55. 
	TEC lock/unlock
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	56. 
	TEC sensor inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	57. 
	Backbone sensors 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	58. 
	Carriage belt condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	59. 
	Main manifold inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	60. 
	AL manifold inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	61. 
	Engine timing correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


E) Picker 

Ensure that the Trendsetter NEWS picker is operating correctly.
Allow 2.5 hours.

	
	Picker
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	
	Picker/Load Table
	
	
	
	
	

	62. 
	Picker up/down cylinders, no leaks/loose jam nuts
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	63. 
	Picker in/out cylinders, no leaks/loose jam nuts
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	64. 
	Wrist cylinders, no leaks/loose jam nuts. 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	65. 
	Picker sensor inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	66. 
	Picker guide cable inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	67. 
	Vacuum cup check, replace if necessary, replace all small fittings and tubes as supplied in kit
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	68. 
	Plate ledge air jets check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	69. 
	Load table plate sensor check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	
	Unload Table
	
	
	
	
	

	70. 
	Table cylinders, no leaks
Clevis’ replaced (if worn at all) and greased
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	71. 
	[Optional] Rotator cylinder, no leaks, proper rotation
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	72. 
	Cup cylinders, no leaks, synchronized motion
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	73. 
	Vacuum cup inspection, replace if necessary
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	74. 
	Traveler and rotator limit switches and sensor check 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	75. 
	Unload table pans inspection
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	76. 
	Unload table optical sensor check
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


F) Workstation

Ensure that the configuration is up to date.
Allow 30 minutes.

	
	Workstation and Controlled Release
	Pass
	Needs
Attn
	6 Months
	12 Months
	Comments

	77. 
	SCSI cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     

	78. 
	Test operation (send 3 jobs in a row from Print Console)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	     


G) Service Comments

Note any:

· Safety features disabled or bypassed

     
· Parts replaced

     
· Firmware and software updates installed

     
· Operating environment issues

     
PM Completion

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	     

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step      
	Date to Complete PM:
	     

	
	Reason:
	     

	
	Plate Count:
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Customer Support
Tel: 604-451-2727
Toll-free: 800-472-2727
callcentre@creo.com
www.creo.com
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