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Trendsetter Upgrade Paths (4-page and 8-page)

If you have a Kodak® 4-page or 8-page Trendsetter®, there are several options available to increase performance and add functionality. Functionality or performance can be increased either by field-installable upgrades or device trade-ins for new or remanufactured devices.

Fill out the information below about your device and find out your upgrade possibilities.

Step 1: Determine What Type of Trendsetter You Have

Fill in the following information to help determine possible upgrades for your Trendsetter.

Serial Number: 
     
See rear of device near power cord.

Generation: 
 FORMCHECKBOX 
 Trendsetter 3230/3244 
See chart below.

 FORMCHECKBOX 
 Trendsetter 400/800

 FORMCHECKBOX 
 Trendsetter 400/800 II

 FORMCHECKBOX 
 Trendsetter 400/800 III


Speed: 
 FORMCHECKBOX 
 S    FORMCHECKBOX 
 F    FORMCHECKBOX 
 V     FORMCHECKBOX 
 X
Current configuration

Format: 
 FORMCHECKBOX 
 4 page       FORMCHECKBOX 
 8 page
Current configuration

Automation: 
 FORMCHECKBOX 
 Base 
Current configuration

 FORMCHECKBOX 
 Autoloader 

 FORMCHECKBOX 
 ContinuousLoad 

Imaging:
 FORMCHECKBOX 
 Quantum
Current configuration


 FORMCHECKBOX 
 Non-Quantum
	Generation
	Serial number
	Dates manufactured
	Notes

	Trendsetter 3230/3244
	S001-S389
	May 1996–May 2000
	Manufactured by Creo

	
	xx3631001- xx3631534
	Oct 1997–May 2000
	Manufactured by Heidelberg

	
	TF01 – TF14
	Dec 1998–Dec 1999
	Manufactured by Creo

	
	xx3710001 – xx3710180
	Dec 1998–May 2000
	Manufactured by Heidelberg

	
	xx3850001 – xx3850119
	Mar 2000–Jul 2001
	Manufactured by Heidelberg

	Trendsetter 400/800
	TE001 – TE820
	Mar 2000–Aug 2003
	Manufactured by Creo 

	
	xx3860001 – xx3860289 
	Mar 2000–Jul 2001
	Manufactured by Heidelberg

	Trendsetter 400/800 II
	TM001 – TM1225
	Jan 2003–Nov 2006
	Manufactured by Creo/Kodak 

	Trendsetter 400/800 III
	TG001 – TGxxxx
	Nov 2006–Present
	Manufactured by Kodak 


Step 2: Identify Upgrade Opportunities

1. Speed Upgrades

4-page and 8-page Trendsetters are classified in the following 4 throughput categories:

· Standard (S)

· Fast (F)

· Very Fast (V) 

· eXtra Fast (X) (available on Trendsetter 800 II or Trendsetter 800 III only and cannot be combined with Spectrum option)

The different Trendsetter generations have evolved over time resulting in different throughput specifications. Please check the table in Appendix A on page 4 to verify the throughput specifications of your current Trendsetter and the upgrade options available to improve the performance.

2. Autoloader Upgrades

The Autoloader option adds plate-handling automation to the 4-page or 8-page Trendsetter with the ability to load up to 80 plates for unattended operation.

Autoloaders are not field-upgradeable. Please contact neijbersen@kodak.com for any Autoloader upgrade requirements.

3. ContinuousLoad Upgrades

This upgrades a Trendsetter base machine to a ContinuousLoad. This upgrade is available on Trendsetter 400/800 II and Trendsetter 400/800 III generation devices only.

4. Quantum Feature Set Upgrade

The Quantum feature set, including a Kodak SQUAREspot® imaging head, thermal compensation, Geometric Correction, and Staccato® 20 Series screening. In combination, these features offer the highest process control and opportunity to deliver high-quality differentiation.

All Trendsetters labeled as Trendsetter 3244 or Trendsetter 3230 have Quantum-equivalent features, with the exception of included Staccato 20 license. The Quantum differentiation began with the Trendsetter 400/800 in Oct 2001 (TE351) and continues to be featured on the Trendsetter 400/800 II and Trendsetter 400/800 III. Any Trendsetter 800 can be upgraded to a Trendsetter 800 Quantum; or a Trendsetter 400 to a Trendsetter 400 Quantum.

5. Format Size Increase
If you have a Trendsetter 3230 or Trendsetter 400, it can be upgraded to an 8-page Trendsetter 3244 or Trendsetter 800. This upgrade is not available on Trendsetter 3230 generation devices within the following serial number ranges:

· TFxxx

· xx371xxxx 

· xx385xxxx 

6. Kodak Sword media upgrade for Trendsetter 3230/3244 (20-watt head only) 

This upgrade is only needed when running Kodak Sword media on a Trendsetter 3230/3244 generation devices with a 20-watt head. The new 20-watt head utilizes a side-looking focus block, which is compatible with imaging Kodak Sword media.

7. Spectrum Proofing Upgrades
Spectrum proofing is no longer available as a field upgrade.
Step 3: Determine Pricing

Contact your local sales representative for further information on available upgrades and pricing.

Appendix A: Speed Upgrades and Throughput Specifications

Trendsetter 8-page configurations

Note: Effective 01 Oct 2007, Trendsetter 3244 Speed Upgrades are at End Of Sales. They will not be available as of 01 Jan 2008.

	Trendsetter generation
	S speed throughput & shipped configuration*
	F speed throughput & shipped configuration*
	V1.0 speed throughput & shipped configuration*

	
	
	
	
	

	Trendsetter 3244
	Base
	9 pph (20-watt head)
	16 pph (20-watt head)


	22 pph (40-watt head)



	
	AL
	10 pph (20-watt head)
	17 pph (20-watt head)


	24 pph (40-watt head)



	Possible upgrade path based on serial number:

	S001 to S161
	S to F (with 20 W air-cooled head)

	S162 to S 389 and xx3631001 to xx3631534
	S to F 

S to V1.0 

F to V1.0 (all upgrades include a 40 W water-cooled head)


	Trendsetter generation
	S speed throughput & shipped configuration*
	F speed throughput & shipped configuration*
	V speed throughput & shipped configuration*

	
	
	
	V1.0
	V2.0

	
	
	
	
	
	

	Trendsetter 800**
	Base
	9 pph (40-watt head)  xx386xxxx shipped with 20-watt head
	16 pph (40-watt head)

xx386xxxx shipped with 20-watt head
	22 pph (40-watt head)

TE001 to TE237
	27 pph (40-watt head)

TE238 and above

	
	AL
	10 pph (40-watt head) xx386xxxx shipped with 20-watt head
	17 pph (40-watt head)

xx386xxxx shipped with 20-watt head
	24 pph (40-watt head)

TE001 to TE237
	30 pph (40-watt head)

TE238 and above

	Possible upgrade path based on serial number:

	TE001 to TE820
	S to F

S to V2.0
F to V2.0

	xx3860001 to xx3860289
	S to F

S to V2.0

F to V2.0 (all upgrades include a 40 W water-cooled head)


	Trendsetter generation
	S speed throughput & shipped configuration*
	F speed throughput & shipped configuration*
	V speed throughput & shipped configuration*
	X speed throughput & shipped configuration*

	
	
	
	
	
	

	Trendsetter 800 II
	Base
	15 pph (40-watt head)
	22 pph (40-watt head)
	30 pph (40-watt head)
	35 pph (50-watt TH2 head)***

	
	CL
	16 pph (40-watt head)
	24 pph (40-watt head)
	34 pph (40-watt head)
	38 pph (50-watt TH2 head)***

	
	AL
	16 pph (40-watt head)
	24 pph (40-watt head)
	34 pph (40-watt head)
	40 pph (50-watt TH2 head)***

	Possible upgrade path based on serial number:

	TM001 and above
	S to F

S to V

F to V

S to X   (includes 50 W TH2 head)

F to X   (includes 50 W TH2 head)

V to X   (includes 50 W TH2 head)


	Trendsetter generation
	S speed throughput & shipped configuration*
	F speed throughput & shipped configuration*
	V speed throughput & shipped configuration*
	X speed throughput & shipped configuration*

	
	
	
	
	
	

	Trendsetter 800 III
	Base
	15 pph (40-watt head)
	22 pph (40-watt head)
	30 pph (40-watt head)
	37 pph (50-watt TH2 head)***

	
	CL
	16 pph (40-watt head)
	24 pph (40-watt head)
	34 pph (40-watt head)
	40 pph (50-watt TH2 head)***

	
	AL
	16 pph (40-watt head)
	24 pph (40-watt head)
	34 pph (40-watt head)
	42 pph (50-watt TH2 head)***

	Possible upgrade path based on serial number:

	TG001 and above
	S to F

S to V

F to V

S to X   (includes 50 W TH2 head)

F to X   (includes 50 W TH2 head)

V to X   (includes 50 W TH2 head)


* Throughputs shown are for 8-page 40.5 inch wide plates. Throughput may vary depending on the media being imaged.

** Early TS800 devices were sold with the TS3244+ model name.

*** The media thickness is limited to 0.20 mm to 0.30 mm (0.008 in. to 0.012 in.) for X speed

Trendsetter 4-page configurations

Note: Effective 01 Oct 2007, Trendsetter 3230 Speed Upgrades are at End Of Sales. They will not be available as of 01 Jan 2008.
	Trendsetter generation
	S speed throughput & shipped configuration*
	F speed throughput & shipped configuration*
	V speed throughput & shipped configuration*

	
	
	
	V1.0
	V2.0

	
	

	Trendsetter 3230


	Base
	11 pph (20-watt head)
	19 pph (20-watt head)
	26 pph (40-watt head)

S162 & above and xx363xxxx
	31 pph (40-watt head)

xx385xxxx

	
	AL
	12 pph (20-watt head)
	21 pph (20-watt head)
	29 pph (40-watt head)

S162 & above and xx363xxxx
	36 pph (40-watt head)

xx385xxxx

	Possible upgrade path based on serial number:

	S162 to S 389 and xx3631001 to xx3631534
	S to V1.0

F to V1.0

	xx3850001 to xx3850119
	S to V2.0

F to V2.0

	TF01 to TF14 and xx3710001 to xx3710180
	No Upgrade is available


	Trendsetter generation
	S speed throughput & shipped configuration*
	V speed throughput & shipped configuration*

	
	
	V1.0
	V2.0

	
	
	
	
	

	Trendsetter 400**
	Base
	11 pph (40-watt head)  xx386xxxx shipped with 20-watt head
	22 pph (40-watt head)

TE001 to TE237
	27 pph (40-watt head)

TE238 and above

	
	AL
	12 pph (40-watt head) xx386xxxx shipped with 20-watt head
	24 pph (40-watt head)

TE001 to TE237
	30 pph (40-watt head)

TE238 and above

	Possible upgrade path based on serial number:

	TE001 to TE820 and xx3860001 to xx3860289
	S to V2.0 


	Trendsetter generation
	S speed throughput & shipped configuration*
	V speed throughput & shipped configuration*

	
	
	
	

	Trendsetter 400 II
	Base
	19 pph (40-watt head)  
	36pph (40-watt head)



	
	CL
	21 pph (40-watt head)
	41 pph (40-watt head)

	
	AL
	21 pph (40-watt head) 
	41 pph (40-watt head)



	Possible upgrade path based on serial number:

	TM001 and above
	S to V


	Trendsetter generation
	V speed throughput & shipped configuration*

	
	
	

	Trendsetter 400 III
	Base
	43 pph (40-watt head)



	
	CL
	50 pph (40-watt head)

	
	AL
	50 pph (40-watt head)



	Possible upgrade path based on serial number:

	TG001 and above
	No upgrade is available


* Throughputs shown are for 4-page 30 inch wide plates. Actual throughput may vary depending on the media being imaged. 

** Early Trendsetter 400 devices were sold with the Trendsetter 3230+ model name. 

About Kodak Graphic Communications Group (GCG)

The leading provider of graphic communications solutions worldwide, Kodak’s Graphic Communications Group (GCG) offers image capture systems; professional color, copydot, and high-speed document scanning systems; inkjet printing and proofing systems; workflow and color management software; thermal imaging devices for film, plates, and proofs; high-quality proofing media, printing plates, and recording film; on-demand color and black-and-white printing systems; data storage products; and professional services. With corporate headquarters located in Rochester, N.Y., Kodak (NYSE: EK) has the largest global sales force and is committed to a digitally oriented growth strategy.  For more information, visit www.graphics.kodak.com.

© Kodak, 2007. Kodak and Trendsetter are trademarks of Kodak.
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