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Customer:
     
Address:
     
Device Serial #:
     
Creo Contact:
     
Date:
     

Trendsetter VLF
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Trendsetter VLF.  Steps that have the greatest impact on system safety and operation appear first in the checklist.

A) Safety and Exterior 

Ensure that the Trendsetter VLF is safe to operate and safe to work on.

	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	1. 
	Right e-stop switch works
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	2. 
	Panels safely interlocked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	3. 
	Chiller fluid not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	4. 
	Debris cabinet hose not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	5. 
	Panels, skins and table in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


B) System Operation 

Evaluate the current operating condition of the Trendsetter VLF.

	
	System Operation
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	6. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	Operator comments summarized below:

	     

	7. 
	Operator trained
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	8. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· Submit a test plot for reference.

	9. 
	P-door moves properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	10. 
	Table vacuum turns on and holds plate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	11. 
	Table moves up/down
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	12. 
	Electronic registration successful
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	13. 
	Plate loads onto drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	14. 
	Plate edge detected
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	15. 
	Carriage moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	16. 
	Plot successful
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	17. 
	Plate unloads from drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


C) Imaging 

Ensure that the image quality is correct and that the imaging system is operating correctly.

	
	Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	Imaging Head
	
	
	
	
	
	
	

	18. 
	Test plot assessed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	19. 
	Stroke reference graph generated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	20. 
	Laser power within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	21. 
	Sum and focus error within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· Remove the thermal imaging head

	22. 
	Debris nozzle checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	23. 
	Lens checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· Re-install the thermal imaging head

	24. 
	Stroke reference graph generated and compared
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	25. 
	Contrast checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	26. 
	Laser power still within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	27. 
	Shutter opens/closes
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	28. 
	Configuration saved
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	29. 
	Data cables replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	
	
	●
	     

	
	Carriage
	
	
	
	
	
	
	

	30. 
	Carriage rails lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	31. 
	Carriage lead screw lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	
	Dehumidifier Unit (DHU)
	
	
	
	
	
	
	

	32. 
	Filter checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	33. 
	Filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	34. 
	Pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· If the pressure indicator is red, the DHU MUST be replaced and the air system examined for contaminants.

	
	Debris Removal Unit
	
	
	
	
	
	
	

	35. 
	Sensor sends correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	36. 
	Filter in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	37. 
	Hose in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Chiller
	
	
	
	
	
	
	

	38. 
	No leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	39. 
	Condenser and air vents cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	40. 
	Pump strainer/ fluid filter cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	41. 
	Pump motor lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	42. 
	Fluid level correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Image Quality
	
	
	
	
	
	
	

	· Submit a second test plot for reference.

	43. 
	Image quality good
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


D) Trendsetter VLF 

Ensure that the Trendsetter VLF system is operating correctly.

	
	Trendsetter VLF
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	Power Box
	
	
	
	
	
	
	

	44. 
	Keyswitch operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	45. 
	Cooling fans run smoothly and quietly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Fan Box
	
	
	
	
	
	
	

	46. 
	Intake air filters clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	47. 
	Compressed air filters clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	48. 
	Air dump operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	49. 
	Air supply pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	50. 
	No air leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Engine
	
	
	
	
	
	
	

	51. 
	Engine timing correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	52. 
	P-door actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	53. 
	Drum and LEC clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	54. 
	Drum straps tight and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	55. 
	Drum belt tensioned properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	56. 
	Encoder disk clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	57. 
	Rollers clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	58. 
	Roller actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	59. 
	Roller pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	60. 
	Roller moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	61. 
	Roller rotates smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	62. 
	TEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	63. 
	TEC pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	64. 
	TEC magnets clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	65. 
	TEC rod ends positioned correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	66. 
	TEC locks/unlocks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	67. 
	TEC sensors send correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	68. 
	Backbone sensors send correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	69. 
	LEC hinge clean 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	70. 
	LEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	71. 
	Backbone actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	72. 
	Carriage fan delivers adequate air flow, quiet
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	73. 
	Carriage belt tensioned properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	74. 
	Main manifold free of leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	75. 
	Table vacuum generator filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	76. 
	Balance weight actuators secure, no leaks, release tips in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	77. 
	Balance weight hall sensors send correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	78. 
	Balance weights lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	79. 
	Balance weight release aligned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	80. 
	Balance weights move smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	81. 
	Engine timing correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Table and P-door
	
	
	
	
	
	
	

	82. 
	Table slide gate opens easily
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	83. 
	Table in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	84. 
	Leading edge straight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	85. 
	Table to LEC distance correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	86. 
	Table tangent to drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	87. 
	Plate drops accurately
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


E) Workstation 

Ensure that the configuration is up to date.

	
	Workstation and Controlled Release
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	88. 
	SCSI cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	89. 
	All software at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	90. 
	All firmware at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	91. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


F) Creo Service Comments

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed

     
Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	     

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step      
	Date to Complete PM:
	     

	
	Reason:
	     

	
	Plate Count:
	     

	
	
	


	Name of Creo representative:
	     

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	     

	Signature:
	 FORMCHECKBOX 


	Date:
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Customer Support
Tel: 604-451-2727
Toll-free: 800-472-2727
callcentre@creo.com
www.creo.com
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