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Customer:
     
Address:
     
Device Serial #:       
Creo Contact:       
Date:
     

Trendsetter VLF Autoloader (SCU, S-Conveyor)
Planned Maintenance Checklist

The objective of Planned Maintenance (PM) is to maximize uptime for the Trendsetter VLF AL.  Steps that have the greatest impact on system safety and operation appear first in the checklist.

A) Safety and Exterior

Ensure that the Trendsetter VLF AL is safe to operate and safe to work on.

	
	Safety First and Exterior Evaluation 
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	1. 
	Guard rail gate locked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	2. 
	Front safety panels secure
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	3. 
	Right e-stop switch works
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	4. 
	Table drop leaf closes safety loop
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	5. 
	Left e-stop switch working
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	6. 
	SSR safety cover closes safety loop
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	7. 
	SSR bin door closes safety loop
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	8. 
	Panels safely interlocked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	9. 
	Rear safety panels in place
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	10. 
	Picker lights on
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	11. 
	Track lights on
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	12. 
	Chariot path unobstructed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	13. 
	Chiller fluid not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	14. 
	Debris cabinet hose not leaking
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	15. 
	Panels, skins and all working surfaces (table, conveyor deck, etc) in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


B) System Operation

Evaluate the current operating condition of the Trendsetter VLF AL.

	
	System Operation
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	16. 
	Operator feedback
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	Operator comments summarized below:

	     

	17. 
	Operator trained
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	18. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· Submit a test plot for reference.

	19. 
	Cassette door opens/closes
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	20. 
	Picker door opens/closes
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	21. 
	Picker moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	22. 
	Picker picks the plate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	23. 
	Slip sheet picker removes the slip sheet
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	24. 
	SSR rollers turn on and pull the slip sheet into the bin
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	25. 
	SSR compactor moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	26. 
	Table cups turn on and hold plate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	27. 
	Plate drops onto table accurately
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	28. 
	Y-axis moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	29. 
	Y-axis gripper grabs and holds the plate securely
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	30. 
	P-door opens/closes
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	31. 
	Table vacuum ports/cups turn on and hold plate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	32. 
	Table moves up/down
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	33. 
	Electronic registration successful
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	34. 
	Plate loads onto drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	35. 
	Plate edge detected
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	36. 
	Carriage moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	37. 
	Plot successful
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	38. 
	Plate unloads from drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	39. 
	Conveyor turns on/off
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


C) Imaging

Ensure that the image quality is correct and that the imaging system is operating correctly.

	
	Imaging
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	Imaging Head
	
	
	
	
	
	
	

	40. 
	Test plot assessed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	41. 
	Stroke reference graph generated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	42. 
	Laser power within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	43. 
	Sum and focus error within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· Remove the thermal imaging head

	44. 
	Debris nozzle checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	45. 
	Lens checked for damage and cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· Re-install the thermal imaging head

	46. 
	Stroke reference graph generated and compared
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	47. 
	Contrast checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	48. 
	Laser power still within spec
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	49. 
	Shutter opens/closes
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	50. 
	Configuration saved
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	51. 
	Data cables replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	
	
	●
	     

	
	Carriage
	
	
	
	
	
	
	

	52. 
	Carriage rails lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	53. 
	Carriage lead screw lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	
	Dehumidifier Unit (DHU)
	
	
	
	
	
	
	

	54. 
	Filter checked
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	55. 
	Filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	56. 
	Pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	· If the pressure indicator is red, the DHU MUST be replaced and the air system examined for contaminants.

	
	Debris Removal Unit
	
	
	
	
	
	
	

	57. 
	Sensor sends correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	58. 
	Filter in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	59. 
	Hose in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Chiller
	
	
	
	
	
	
	

	60. 
	No leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	61. 
	Condenser and air vents cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	62. 
	Pump strainer/ fluid filter cleaned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	63. 
	Pump motor lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	64. 
	Fluid level correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Image Quality
	
	
	
	
	
	
	

	· Submit a second test plot for reference.

	65. 
	Image quality good
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


D) Trendsetter VLF

Ensure that the Trendsetter VLF system is operating correctly.

	
	Trendsetter VLF
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	Power Box
	
	
	
	
	
	
	

	66. 
	Keyswitch operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	67. 
	Circuit board warning lights off
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	68. 
	Cooling fans run smoothly and quietly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Fan Box
	
	
	
	
	
	
	

	69. 
	Intake air filters clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	70. 
	Compressed air filters clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	71. 
	Air dump operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	72. 
	Air supply pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	73. 
	No air leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Engine
	
	
	
	
	
	
	

	74. 
	Engine timing correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	75. 
	P-door actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	76. 
	Drum and LEC clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	77. 
	Drum straps tight and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	78. 
	Drum belt tensioned properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	79. 
	Encoder disk clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	80. 
	Rollers clean and in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	81. 
	Roller actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	82. 
	Roller pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	83. 
	Roller moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	84. 
	Roller rotates smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	85. 
	TEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	86. 
	TEC pressure adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	87. 
	TEC magnets clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	88. 
	TEC rod ends positioned correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	89. 
	TEC locks/unlocks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	90. 
	TEC sensors send correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	91. 
	Backbone sensors send correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	92. 
	LEC hinge clean
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	93. 
	LEC actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	94. 
	Backbone actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	95. 
	Carriage fan delivers adequate air flow, quiet
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	96. 
	Carriage belt tensioned properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	97. 
	Main manifold free of leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	98. 
	AL manifold free of leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	99. 
	Table vacuum generator filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	100. 
	Balance weight actuators secure, no leaks, release tips in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	101. 
	Balance weight hall sensors send correct signal
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	102. 
	Balance weights lubricated
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	103. 
	Balance weight release aligned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	104. 
	Balanced weights move smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	105. 
	Engine timing correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	Table, P-door,Y-axis
	
	
	
	
	
	
	

	106. 
	Guard rail gate opens easily and latches securely
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	107. 
	Load/unload vacuum adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	108. 
	Load/unload vacuum cups (black) replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	109. 
	Plate transfer vacuum adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	110. 
	Plate transfer vacuum cups (red) replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	111. 
	Table drop leaf opens easily and latches securely
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	112. 
	Table in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	113. 
	X-axis tape smooth and well adhered
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	114. 
	Table flat
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	115. 
	Bumpers contact the table evenly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	116. 
	Leading edge straight
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	117. 
	Table to LEC distance correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	118. 
	Table tangent to drum
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	119. 
	Table dampers secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	120. 
	Plate drops accurately
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	121. 
	Y-axis grips securely and moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	122. 
	Y-axis gripper aligned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	123. 
	Y-axis home position correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


E) Autoloader

Ensure that the Autoloader system is operating correctly.

	
	Autoloader
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	
	Picker and Track
	
	
	
	
	
	
	

	124. 
	Track belt tensioned properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	125. 
	Picker height to plenum correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	126. 
	Circuit board warning lights off
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	127. 
	Manifold free of leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	128. 
	Picker deck vacuum generator filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	129. 
	P-cups clean, move properly 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	130. 
	Lift arm moves properly, in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	131. 
	Lift arm actuator secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	132. 
	Vacuum cups (green) clean, move properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	133. 
	Vacuum cups (green) replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	134. 
	Eject/pusher fingers clean, move properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	135. 
	Eject finger actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	136. 
	Slip sheet picker clean, moves smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	137. 
	Slip sheet picker actuator secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	138. 
	Slip sheet picker cups move smoothly, aligned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	139. 
	Slip sheet picker belts tensioned properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	140. 
	Slip sheet picker vacuum adequate
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	141. 
	Slip sheet picker vacuum generator filter replaced
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	
	
	
	
	
	
	
	
	

	
	Single Cassette Unit (SCU)
	
	
	
	
	
	
	

	142. 
	All circuit board warning lights off
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	143. 
	Manifold free of leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	144. 
	Cassette doors move smoothly and symmetrically
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	145. 
	Cassette to plenum height correct
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	146. 
	Cassette/cart latches smoothly, securely
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	147. 
	Cassette/cart castors secure, in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	148. 
	Cassette cover light tight, opens/closes smoothly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	149. 
	Media centered in cassette
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	150. 
	Reflective tape smooth, well adhered
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	
	Slip Sheet Removal Unit (SSR)
	
	
	
	
	
	
	

	151. 
	Rollers open properly, in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	152. 
	Rollers aligned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	153. 
	Roller shields have adequate clearance from rollers
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	154. 
	Roller actuators secure, no leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	155. 
	Rollers and motor aligned
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	156. 
	Manifold free of leaks
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	157. 
	Compactor operates correctly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	
	S Conveyor
	
	
	
	
	
	
	

	158. 
	Circuit board warning lights off
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	159. 
	Belts tensioned properly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	●
	
	●
	     

	160. 
	Speed matches the processor
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


F) Workstation

Ensure that the configuration is up to date.

	
	Workstation and Controlled Release
	Pass
	Needs
Attn
	6 Months
	12 Months
	18 Months
	24 Months
	Comments

	161. 
	SCSI cable and connections in good condition
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	162. 
	All software at latest version 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	163. 
	All firmware at latest version
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     

	164. 
	Settings backed up
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	●
	●
	●
	●
	     


G) Creo Service Comments

Note any:

· Safety features disabled or bypassed

· Parts replaced

· Firmware and software updates installed

· Operating environment issues

· FCOs installed

     
Customer Acceptance

	 FORMCHECKBOX 
  PM is complete
	Next PM date:
	     

	
	
	

	 FORMCHECKBOX 
  PM is partially complete to step       
	Date to Complete PM:
	     

	
	Reason:
	     

	
	Plate Count:
	     

	
	
	


	Name of Creo representative:
	     

	Signature:
	 FORMCHECKBOX 



	Name of Customer representative:
	     

	Signature:
	 FORMCHECKBOX 


	Date:
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Customer Support
Tel: 604-451-2727
Toll-free: 800-472-2727
callcentre@creo.com
www.creo.com
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