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Overview

Upon installation of Brisque 5.x, the Kodak service engineer performs an installation test procedure checklist (ITPC), which is a series of tests devised to demonstrate that the installation has been successfully completed.

The Kodak service engineer must complete the installation test checklist after performing all the test procedures described in “System Test Procedure” on page 5.

The ITP usually takes between 2 and 3 hours to complete. 

When the tests have been successfully completed, Brisque 5.x is ready for ongoing production work with the full support of the Kodak customer service department.

Customer Responsibilities

The customer is responsible for the following: 

· There must be a sufficient supply of media for proofing and plates.

· Customer is responsible for providing proper network infrastructure according to Kodak standards and requirements.

· One customer representative must be present during the ITPC.

Kodak Responsibilities

Kodak is responsible for the following:

· The Brisque software and any necessary hardware must be fully installed and integrated, including integrating and testing the output devices where applicable.

· Brisque v5.0/5.1 client must be installed on a Macintosh computer or Windows operating system client platform.

· After installing Brisque, the product must be explained to the customer so that the customer is able to understand and follow the ITPC.

Any additional system, workflow, color calibration, or Staccato screening calibration on press are not part of the ITP, and are not covered in this checklist. 

If the Test Fails

The Kodak service engineer checks all of the configuration settings if the test fails. If the problem is not related to the installation and configuration, the Kodak service engineer will open a support call. The warranty period will not begin until the problem is solved.

If a problem occurs when the ITP is performed after installation and without Kodak assistance, contact the Kodak Response Center.

System Details

	Brisque configuration name 
(select: Tools > System Tools > Station Information)
	Expose / Access / Pro / Impose      

	Platform configuration
	Platform type      
RAM     
Communication Gigabit / 100BaseT / 10BaseT / Other

	Client configuration
	Windows (configuration)      
Macintosh (configuration)      


Output Devices to be Tested

List the output devices specified during the sales process:

	Single-page proofer
	Imposition proofer
	Final output

	
	
	

	
	
	


Test Procedure Checklist

The Kodak service engineer must complete this test procedure checklist, after performing all of the test procedures (as described in the "System Test Procedure" section).

	Tasks
	Completed

	Creation of Templates and Hot Folders
	 FORMCHECKBOX 


	Job creation and page RIP
	 FORMCHECKBOX 


	Resource Center and Preferences
	 FORMCHECKBOX 


	ICF translation, editing impositions and page assignment
	 FORMCHECKBOX 


	Proofing and final output
	 FORMCHECKBOX 


	Mounting file server(s) or other Brisque stations over NFS
	 FORMCHECKBOX 


	System tools and maintenance
	 FORMCHECKBOX 


	Remote access to system via RSS

	 FORMCHECKBOX 



Customer Comments

Note any customer comments or actions needed:

	     


Confirmation

The installation test was performed on   /   /     (day/month/year) by a representative of Kodak and witnessed by at least one representative of the customer.

	Kodak representative:
	     

	Signature:
	


	Customer representative:
	

	Signature:
	


Upon completion of this checklist, the Kodak service engineer will send a copy of the entire document to the regional service manager.

System Test Procedure

Before running the installation test procedure:

· Ensure that the workflow is in working order, including all of the entitled output devices. 

· Ensure that each process to be tracked has a unique process template.

· Ensure that the v5.1 client was installed on the Macintosh/Windows client workstation 

Locate the Installation Test Procedure Files

	Step
	Comment

	Locate the installation test procedure files. 
	These files are usually located in the ITP folder of your installation CD.

	Check
	 FORMCHECKBOX 



Creation of Templates and Hot Folders

	Step
	Comment

	1. From a Macintosh or Windows client station, log on to the Brisque workstation as an administrator (password is not required).
	The Host table of the Mac/Windows client workstation must be modified, and contain the Brisque host name and IP address, to enable login using the Brisque host name.

	Check
	
	 FORMCHECKBOX 


	2. Create a new Template that will include: PreFlight Check > RIP > FAF > Preview, and assign it to a new Hot Folder. Name the Hot Folder: RIP_HF
	The RIP Hot Folder must include an AppleTalk Printer—this is required for the next ITP test, Printing page from QuarkXPress or InDesign.

Note: Applicable for types of Brisque that support RIP and FAF.



	Check
	 FORMCHECKBOX 


	3. Copy a Postscript file from the Samples Folder (located in the ITP Directory) to the newly created Hot Folder.
	Make sure all steps are performed correctly.
	

	Check
	 FORMCHECKBOX 



	4. Create a new Hot Folder that will include: Translate > ImpoCheck > Preview > PlateExpose. Name the Hot Folder: Impo_HF
	Note: Translate is for Brisque Impose only.

	

	Check
	 FORMCHECKBOX 



Job Creation and Page RIP

	Step
	Comment

	1. Print a file from QuarkXPress software or Adobe InDesign software to the RIP_HF Hot Folder.
	Verify that process starts and finishes correctly.
	

	Check
	 FORMCHECKBOX 


	2. Using Preview, verify that the file was RIPed correctly.
	Make sure that all pages contain all the expected data.
	

	Check
	 FORMCHECKBOX 


	3. After mounting the Brisque volume on the Mac desktop, repeat the above step with a PDF copied to the RIP_HF Hot Folder via AppleTalk.
	HELIOS license must be installed (a permanent or demo license).
	

	Check
	 FORMCHECKBOX 



Resource Center and Preferences

	Step
	Comment

	1. Open the Marks category and add a mark. Modify the mark parameter so it is exposed only with the Black separation.
	Close the Resource Center and then reopen to verify that the settings are saved. Verify that the imported mark is used for the Imposition test.
	

	Check
	 FORMCHECKBOX 


	2. Create a new PreFlight Check profile according to the customer’s needs.
	Show the customer how to open the Online Help to learn about Profile settings.
	

	Check
	 FORMCHECKBOX 



	Step
	Comment

	3. Open Preferences (under the Edit menu) and create a new user.
	Make sure that the customer knows how to create a user for each operator. Check the user permissions (admin/regular).
	

	Check
	 FORMCHECKBOX 


	4. In Preferences, define Adobe Acrobat software as the File Editor for PDFs.
	
	

	Check
	 FORMCHECKBOX 



ICF Translation, Editing Impositions and Page Assignment (Optional)

Important note: This section is required only for Brisque Impose configurations.

Preparation: Ensure that Preps has been properly set up on the Brisque workflow and copy the Marks library to the correct location in Brisque so that the marks are available in the Resource Center.

	Step
	Comment

	1. RIP the files (PS or PFDs) that are required for the Imposition plan via Preps.
	
	

	Check
	 FORMCHECKBOX 


	2. Print the imposition plan (ICF) from Preps into the Impo_HF Hot Folder.
	
	

	Check
	 FORMCHECKBOX 


	3. Verify that the Imposition previews correctly.
	Verify that all pages and marks exist.
	

	Check
	 FORMCHECKBOX 


	4. Replace one page with a new page via preps, and print the job again.
	Check results.
	

	Check
	 FORMCHECKBOX 



Proofing and Final Output

Preparation:
· Make sure that all output devices are configured and up-to-date, including for example, Press Formats, Screen Sets, and curves.

· Make sure that you can open the Screen Set list of the output device by right clicking the device name in the Monitor palette. 
Note: This shortcut will not work if you used the Brisque IP Address in the Host field when you logged into the system.

	Step
	Comment

	1. Manually proof one page of the job to the Iris/Veris.
	Verify results
	

	Check
	 FORMCHECKBOX 


	2. Improof the Impo Job to the Improof device.
	Make sure results are correct.
	

	Check
	 FORMCHECKBOX 


	3. Expose the same Imp job to a platesetter.
	Verify that the correct plates are loaded.

Select the Update the Plate Remake Database checkbox in the Plate Expose dialog box before exposing.
	

	Check
	 FORMCHECKBOX 


	4. Open the Plate Remake database and locate the job that you have just exposed, and re-expose the Black separation.
	Verify that the exposure results are consistent.
	

	Check
	 FORMCHECKBOX 



Mounting the Server

Preparation:
· Make sure that all existing file servers (Server and other Brisque workstations) are defined in the /etc/hosts file. If necessary, use smit to define the file servers.

	Step
	Comment

	1. Open the File Browser and click the Mount button. From the list, select the file server station and press <Enter>. Select the volume to be mounted and click the Mount button.
	Make sure that the customer knows that the <Enter> key must be pressed after selecting the remote file server station from the list
	

	Check
	 FORMCHECKBOX 


	2. Copy files/folders from the Brisque to the server.
	Use Copy & Paste, and make sure the Copy speed is adequate.

	

	Check
	 FORMCHECKBOX 



System Tools and Maintenance

	Step
	Comment

	1. Open System Tools (under the Tools menu) and create a Brisque Log.
Explain to the customer that this is a very important troubleshooting tool that should be used immediately when they confront a problem.
	Show the customer how to perform this operation. Review the report and check if there is something that is suspected to be incorrect. (For example, if there two entries in the host table for one host name). Send the report to Product Support.


	

	Check
	 FORMCHECKBOX 


	2. Open System Tools (under the Tools menu) and run the Test Local Network.
Explain to the customer that this is a very important troubleshooting tool that should be used whenever a client network throughput is in question
	Show the customer how to perform this operation. Make sure that the network throughput from the client to other host is above 6 MB/sec.


	

	Check
	 FORMCHECKBOX 


	3. Show the customer how to export a Template, a Screen Set and a PreFlight Profile.
	This is required so that all Brisque workstations on the site share the same parameter.
	

	Check
	 FORMCHECKBOX 


	4. Select Scismit > Problem Determination and run the Check Net Performances option.
	You need to provide the IP Address of a remote machine that runs NFS.  Verify that the obtained transfer rates are above 15 MB per sec for Gigabit, and above 5 MB per sec for 100BaseT network card.

If no other machines are running NFS on site, skip this test.
	

	Check
	 FORMCHECKBOX 


	5. Select Scismit > Problem Determinations.
	Show the customer how to perform weekly maintenance.
	

	Check
	 FORMCHECKBOX 


	6. Check the minimum data Volumes throughput.
	Run datavol-test.sh. and verify that the result is above 30 MB/sec.
	

	Check
	 FORMCHECKBOX 


	7. Support: Remote Access to System (RSS)

Contact the Kodak Response Center to test access to the system.

	Depending on the installation, this can be a broadband or modem connection.
	

	Check
	 FORMCHECKBOX 
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� Depending on the availability of a dedicated Analog/ISDN line. Not performing this step should not mark the ITP as FAILED.


� Please note that the Kodak Response Center requires some lead time to test the Remote Access to System via RSS
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