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ECO #	�� FORMTEXT ��B342���Description: �� FORMTEXT ��Incorrect Wording on Laser Hazard sticker���Product affected:�� FORMTEXT ��VLFTS���Priority:�� FORMDROPDOWN ����Action:�� FORMTEXT ��Replace sticker���Machines affected:�� FORMTEXT ��BB1-BB09���Installation time:�� FORMTEXT ��0.25 hr.���List Price:�� FORMTEXT ��–––––���Release Date:�� FORMTEXT ��02/06/97���

Detailed Description:

� FORMTEXT ��The 74-3085A IR Laser Hazard Danger label is replaced with the 74-3145A Interlock Defeated label because the wording is correct. This label is used on the 02-3101A (5080) and 02-3103A (5880) VLF Trendsetters.�



Special tools required:

� FORMTEXT ��none�



Parts needed:  � FORMTEXT ��74-3145A�



Part no.�Description�Quantity��� FORMTEXT ��74-3145A��� FORMTEXT ��Label,Danger,IR Laser Hazard��� FORMTEXT ��6���� FORMTEXT ��–––––��� FORMTEXT ��–––––��� FORMTEXT ��–––––���� FORMTEXT ��–––––��� FORMTEXT ��–––––��� FORMTEXT ��–––––���� FORMTEXT ��–––––��� FORMTEXT ��–––––��� FORMTEXT ��–––––���� FORMTEXT ��–––––��� FORMTEXT ��–––––��� FORMTEXT ��–––––���� FORMTEXT ��–––––��� FORMTEXT ��–––––��� FORMTEXT ��–––––���� FORMTEXT ��–––––��� FORMTEXT ��–––––��� FORMTEXT ��–––––���

Version changes:

Part Changed (Description)�Old Version�New version��� FORMTEXT ��02-3101A��� FORMTEXT ��C��� FORMTEXT ��D���� FORMTEXT ��02-3103A��� FORMTEXT ��B��� FORMTEXT ��C���� FORMTEXT ��74-3042A��� FORMTEXT ��A��� FORMTEXT ��Inactive���

Version change notes:  � FORMTEXT ��–––––�

Old Parts: � FORMTEXT ��74-3042�

Procedure:

� FORMTEXT ��Open each of the six interlock protected door panels ( These are right and left side panels, two rear panels, fan box panel (front left), and front centre panel) and locate the door interlock switches mounted on the Trendsetter frame. Find the old Laser Hazard labels located near the interlock switches and place the new stickers (74-3145A) over the old ones. �
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